2014 LRAUV Configurations for CANON
1. Daphne[image: ]
a. Mission: Circles Makai, or CPF using USBL collecting contextual bio/geo data.  Position tracked by Tiny (WaveGlider), responds to a-comms command to continue mission
b. Instruments:
i. Linquest DVL Serial #013245, LCB B5 (5A)
ii. Benthos DAT Serial # XXXX, LCB B6
iii. Wetlabs Puck Serial # XXXX, LCB B3
iv. NBOSI CTD Serial # XXXX, LCB B4
v. Turner Cyclops Rhodamine , Serial # XXXX ,LCB B0 (A/D)
vi. Sparton Compass, Serial # XXXX , LCB B7
vii. Aanderra Optode Serial # XXXX, not used
viii. MBARI ISUS Serial # XXXX, LCB B1
ix. MBARI SCIPI, Serial # XXXX, LCB B2
x. OPEN LCB:  none
c. Comms
i. Freewave, Serial # XXXX  LCB A2
ii. NAL 9602, Serial # XXXX,  LCB A1
iii. Applied Acoustic transducer, Serial 2093573, standalone with 9v batteries, HPR3 Channel 6 (24.038 interrogate, 27.173 kHz reply) 
iv. Desert Star Argos, # 804, ID 136622, standalone battery powered
v. Telonics VHF beacon, Serial #678951A,159.65 MHz, Standalone battery powered
d. Notes: 
2. Tethys[image: ]
a. Mission: Patch tracking with rhodamine sensor, area recon, high resolution data upload (including ADCP?) through hotspot
b. Instruments:
i. Rowe ADCP/DVL Serial #013245, LCB B5 (5A)
ii. Wetlabs Puck Serial # XXXX, LCB B3
iii. Turner Cyclops Rhodamine, Serial # XXXXXX, LCB B0, using PAR port and wiring
iv. NBOSI CTD Serial #XXXXX, LCB B4
v. PNI Compass (in Rowe), Serial #XXXXX, LCB B7
vi. Aanderra 4830 Optode Serial # 240, LCB B2
vii. MBARI ISUS Serial #XXXX , LCB B1
viii. OPEN LCB: B6
c. Comms
i. CDMA radio, Serial #XXX LCB A2, IP 166.248.105.035, 831-710-7016
ii. NAL 9602, Serial #XXX, IMEI 30023401186620, LCB A1
iii. [bookmark: _GoBack]Benthos transponder, Serial # 49897, 26/29 kHz 
iv. Desert Star Argos, Serial # 1022, ID 136621
v. Telonics VHF beacon, Serial #678950A, 159.55 MHz
d. Notes:  
3. Makai[image: ]
a. Mission: Sampler/ Patch center marker Vehicle, holding at density 1025.5, or temperature
b. Instruments
i. Linquest DVL Serial #,10089, LCB B5 (5A)
ii. Benthos modem Serial #XXX, LCB B6
iii. Wetlabs Puck Serial #XXX, LCB B3
iv. NBOSI CTD Serial #XXX, LCB B4
v. Turner Cyclops Rhodamine, Serial #XXX, LCB B0
vi. Sparton Compass, Serial #XXX LCB B7
vii. Aanderra Optode Serial #XXX, LCB B2
viii. OPEN LCB: B1
c. Comms
i. Cradlepoint radio, Serial #XXX LCB A2
ii. NAL 9602, Serial #XXX, LCB A1
iii. Benthos transponder Serial #XXX, 26/29 kHz, standalone battery  
iv. Desert Star Argos Serial # 939, Argos ID 136623, standalone battery 
v. Telonics VHF beacon, Serial #XXX, XXX MHz, standalone battery 
d. Notes: Using MB 2.0, old LCB backplane, new battery pack, new umbilical/charger box, though no shore-power
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