2014 LRAUV Configurations for CANON
1. Daphne [image: ]
a. Mission: Circles Makai, or CPF using USBL collecting contextual bio/geo data.  Position tracked by Tiny (WaveGlider), responds to a-comms command to continue mission
b. Instruments:
i. Linquest DVL Serial #013245, LCB B5 (5A)
ii. Benthos DAT Serial # XXXX, LCB B6
iii. Wetlabs Puck Serial # XXXX, LCB B3
iv. NBOSI CTD Serial # XXXX, LCB B4  
v. PAR , Serial # XXXX, LCB B0 (A/D), LCB A0
vi. Sparton Compass, Serial # XXXX , LCB B7
vii. Aanderra Optode Serial # XXXX LCB B2
viii. MBARI ISUS Serial # XXXX, LCB B1
ix. OPEN LCB:  none
c. Comms
i. Freewave, Serial # XXXX  LCB A2
ii. NAL 9602, Serial # XXXX,  LCB A1
iii.  Applied Acoustic transducer, Serial 2093573, standalone with 9v batteries, HPR3 Channel 6 (24.038 interrogate, 27.173 kHz reply) HPR3 Channel 6 (24.038 interrogate, 27.173 kHz reply) 
iv. Desert Star Argos, # 804, ID 136622 standalone battery powered
v. Telonic VHF beacon#678951A,159.65 MHz, Standalone battery powered
vi. 
d. Notes: 
2. Tethys[image: ]
a. Mission: Patch tracking with rhodamine sensor, area recon, high resolution data upload through hotspot
b. Instruments:
i. Rowe ADCP/DVL Serial #013245, LCB B5 (5A)
ii. Wetlabs Puck Serial # XXXX, LCB B3
iii. Turner Cyclops Rhodamine, Serial # 2180551, LCB B0, using PAR port and wiring
iv. NBOSI CTD Serial #XXXXX, LCB B4
v. PNI Compass (in Rowe), Serial #XXXXX, LCB B7
vi. Aanderra Optode Serial # 241, LCB B2
vii. MBARI ISUS Serial #XXXX , LCB B1
viii. OPEN LCB: B6
c. Comms
i. CDMA radio, Serial #XXX LCB A2
ii. NAL 9602, Serial #XXXLCB A1
iii. Benthos transponder 26/29 kHz , Serial # 49897, 26/29 kHz 
iv. Desert Star Argos, Serial # 1022, ID 136621
v. Telonics VHF beacon, Serial #678950A, 159.55 MHz
d. Notes:  
3. Makai[image: ]
a. Mission: Sampler/ Patch center marker Vehicle, holding at density 1025.5, or temperature
b. Loads
i. Turner Cyclops Rhodamine, Serial #2180550, LCB B0
ii. NBOSI CTD Serial #XXX, LCB B1
iii. Sparton Compass, Serial #XXX LCB B2
iv. NAL 9602, Serial #xxx1590, LCB B3
v. Wetlabs Puck Serial #1073, LCB B4
vi. Aanderra Optode Serial #241, LCB B5 
vii. Cradlepoint radio, Serial #130489900096 LCB B6
viii. ESP, LCB B7 (5A)
ix. Keller Depth Sensor, Serial 51, A0
x. Linquest DVL Serial #,10089, A1 (5A)
xi. Benthos modem Serial #XXX, LCB A2
xii. Mass Shifter, LCB A3
xiii. Elevator, LCB A4
xiv. Rudder, LCB A5
xv. Variable Buoyancy, LCB A6 (5A)
xvi. Thruster, LCB A7 (5A)
c. Comms
i. [bookmark: _GoBack]Benthos transponder Serial #54143, 26/29 kHz
ii. Desert Star Argos Serial # 939, Argos ID 136623
iii. Telonics VHF beacon, Serial #678952, XXX MHz
d. Notes: Using MB 2.0, old LCB backplane, new battery pack, new umbilical/charger box, though no shore-power
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