	Name
	Collection Configuration
	# of Samples
	Total Collection Area (m²)
	Opening/
Closing
	Buoyancy
	Max Operational Depth (m)
	Reference

	Neutrally - Buoyant Sediment Trap (NBST)
	cylinder
	4
	0.0171
	closing (recovery)
	volume changer (VOCHA)
	500m
	Valdes and Price, 2000

	PELAGRA
(Particle Export Lagrangian Trap)
	unsymmetrical funnel
	4
	0.46
	closing (recovery)
	APEX float
	600m
	Lampitt et al. 2008

	Lagrangian Sediment Trap (LST)
	symmetrical funnel
	4
	0.32
	opening closing
	SOLO float
	1500m?
	This Study


Comparison of Free-drifting neutrally buoyant sediment traps.
