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Falmouth Scientific Inc

NXIC-CTD-ADC

S/N 2112 Configuration

Mechanical:

Sensor Endcap:
 FORMDROPDOWN 
 with piston and face seal o-rings

Connector Endcap:
 FORMDROPDOWN 
 with piston and face seal o-rings

Pressure compensation:
 FORMDROPDOWN 

Overall Depth Rating
500 Meters depth limit

Electrical:

Communications:

ASCII Command Port: 
 FORMDROPDOWN 

BAUD:
115200

DATA BITS:
8

STOP BITS:
1

MEMORY:
 FORMDROPDOWN 

Power:

	Sensor
	External power

12 VDC 
	Battery Power

@ 2.5VDC
	

	Options Off
	48
	137
	mA

	All Sensors
	113
	370
	mA

	Sensor A
	     
	     
	mA

	Sensor B
	113
	370
	mA

	Sensor C
	     
	     
	mA

	Sensor D
	     
	     
	mA

	Sensor E
	N/A Internal Power
	N/A Internal Power
	mA


      Use Battery Power @ 2.5VDC current for battery life calculations 

Sensors:
Conductivity:

NXIC type: 
0 to 90 mS/cm²

Thermometer:

Thermistor 100mS:
-5 to +45 ºC

Pressure:



Druck:
0 to 750 psia temp compensated strain gauge bridge

Falmouth Scientific Inc

NXIC-CTD-ADC

S/N 2112 Configuration

SENSOR CONNECTORS WIRING:

	OPTIONS CONNECTOR 1

	POSITION
	PIN #
	SIGNAL
	CHANNEL
	CHANNEL ID

	 FORMDROPDOWN 

	1
	Ground
	DC1
	     

	   Product Name
	2
	Signal (0-5VDC)
	
	

	   Model Number
	3
	+12 V Power
	
	

	   Serial Number
	4
	Signal GND
	
	

	
	5
	Gain0_0
	
	

	
	6
	Gain0_1
	
	

	 FORMDROPDOWN 

	7
	Ground
	DC2
	6

	   Wetlabs Fluorometer
	8
	Signal (0-5VDC)
	
	

	   ECO FL
	9
	+12 V Power
	
	

	   FLRT-872
	10
	Signal GND
	
	

	
	11
	Gain1_0
	
	

	
	12
	Gain1_1
	
	

	
	
	
	

	OPTIONS CONNECTOR 2

	POSITION
	PIN #
	SIGNAL
	CHANNEL
	CHANNEL ID

	 FORMDROPDOWN 

	1
	Ground
	DC3
	     

	   Product Name
	2
	Signal (0-5VDC)
	
	

	   Model Number
	3
	+12V power
	
	

	   Serial Number
	4
	Signal GND
	
	

	Open
	5
	Ground
	DC4
	     

	   Product Name
	6
	Signal (0-5VDC)
	
	

	   Model Number
	7
	+12V power
	
	

	   Serial Number
	8
	Signal GND
	
	

	Flowmeter
	9
	Ground
	RS-232
	23

	   G.O. Environmental
	10
	RXD Received Data
	
	

	   2135D/20314
	11
	Power +12V
	
	

	   B 22360
	12
	TXD Transmitted Data
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