01/29/2016

Topics:
· Canyon Status
· Event 12/1/15: Smaller, logged by BED 2,5. BED 4 broke free. 
· Event 01/15/16: Larger, AMT knocked down?, subsea moorings cut free, 2 BEDs broke free, 2 STEDS released/recovered. 

· BEDs Current Status
· BED 1: Not responding at last known location
· BED 2 (AMT): Not responding at deployed location
· BED 3: Recovered 1/19/16 Lake Moran Beach in SC
· BED 4 (RIP). Search summary: \\atlas.shore.mbari.org\ProjectLibrary\901006.BEDS\update docs\BED_4_search_12_2015
· BED 5: Not responding at last known location
· BED 6: Recovered 1/27/16 by F/V

· Issues
· Data transfer protocol
· Eric slated to begin work. Did cruise to initially quantify problem. 
· Ballast release failures
· Not surviving strong events
· Automatic
·  burnwire option?
· Use larger GTR with increased time release (2 years ok)
· Multi week lead time
· Surface location subsystem
· Best case wasn’t even working. 0/3 so far. 
· Use STEDS unit?
· Use STEDS Argos unit
· CF Card Failures
· Works again once re-inserted 
· Shore-side test simulating floating unit? Moor? 
· Use xyz table to simulate motion
· Use existing BED that has many events on it and has already exhibited failure
· Use G10 material and/or cable tie
· Pressure sensor A/D scaling
· Re-run matlab
· Pressure Sensor Sampling Freq
· Settling timeout too long?
· 1 sec PO (settling) timeout
· Data
· Event Specific
· \\atlas.shore.mbari.org\ProjectLibrary\901006.BEDS\BEDS.Data\CanyonEvents
· Deployment Specific
· \\atlas.shore.mbari.org\ProjectLibrary\901006.BEDS\BEDS.Data\Deployment_Data_Full
· Cruise Specific (Health and Status of Events)
· \\atlas.shore.mbari.org\ProjectLibrary\901006.BEDS\BEDS.Data\Cruise Data\2016
· STOQS:
· http://stoqs.shore.mbari.org:8000/stoqs_cce2015
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Misc:
· Config sheet for CCE acoustics – COMPLETE
· Add new homer IDs to acoustics inventory sheet - Brian

Cruises:


