07/15/2016

Topics:
· Canyon Status
· Event 12/1/15: Smaller, logged by BED 2,5. BED 4 broke free. 
· Event 01/15/16: Larger, AMT knocked down, subsea moorings cut free, 2 BEDs broke free, 2 STEDS released/recovered. 
· Event 02/17/16
· Event 03/06/16
· Possible localized events in the upper canyon. Need to check on BEDs. Nov 16, Dec 23-26. 

· BEDs Current Status
· BED 1: Not responding at last known location
· BED 2 (AMT): Not responding at deployed location. Not on AMT frame. 
· BED 3: Recovered Carson 4/25. 3ml seawater found inside. Full data recovered. 
· BED 4 FOUND! Search summary: \\atlas.shore.mbari.org\ProjectLibrary\901006.BEDS\update docs\BED_4_search_12_2015
· BED 5: FOUND! Decimated data recovered
· BED 6: Deployed
· BED 9: Deployed healthy, no events as of 4/27
· BED 10: Deployed healthy, no events as of 4/27

· To Do
· SAR for BED #2 from AMT site up canyon
· Check in with BED 6 and 5.
· Fix BED #8
· October 5, 2016 target deployment date. Deploy 3 BEDs in spheres and one on AMT. 
· WG cruise mid-september to locate. 
· Pursue anti-roll attachment
· Investigate .WAT files being put into STOQS
· [bookmark: _GoBack]Pull .WAT files for BED#5. Charlie/Roberto to send dates and times for .WAT data. 

· Procurement
· Done. No $ left

· Issues
· Prevo leaks?
· Test in pressure bomb? Larry?
· Data transfer protocol
· Eric slated to begin work. Did cruise to initially quantify problem. 
· 04/2016 – Great progress was made by Eric. Downloads are now possible unattended from the Waveglider. 
· Ballast release failures
· Not surviving strong events
· Larger GTR and the “Larry GTR” seems to be working better. 
· Surface location subsystem
· Using new Telonics tags now. 
· CF Card Failures
· Works again once re-inserted 
· Still logging data even though it’s saying that it can’t. Only seems to occur with high humidity. 
· Shore-side test simulating floating unit? Moor? 
· Use xyz table to simulate motion
· Use existing BED that has many events on it and has already exhibited failure
· Use G10 material and/or cable tie
· Pressure sensor A/D scaling
· Re-run matlab
· Pressure Sensor Sampling Freq
· Settling timeout too long?
· 1 sec PO (settling) timeout
· Data
· Event Specific
· \\atlas.shore.mbari.org\ProjectLibrary\901006.BEDS\BEDS.Data\CanyonEvents
· Deployment Specific
· \\atlas.shore.mbari.org\ProjectLibrary\901006.BEDS\BEDS.Data\Deployment_Data_Full
· Cruise Specific (Health and Status of Events)
· \\atlas.shore.mbari.org\ProjectLibrary\901006.BEDS\BEDS.Data\Cruise Data\2016
· STOQS:
· http://stoqs.shore.mbari.org:8000/stoqs_cce2015


Misc:
· Config sheet for CCE acoustics – COMPLETE
· Add new homer IDs to acoustics inventory sheet - Brian

Cruises:


