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About the IMU: The IMU needs to be calibrated for best functionality. It needs to be moved around a bit, there are some notes at the end of the document I sent (attached).

Mostly the goal is to show each of the six sides of the board to the sky and keep it steady enough for the unit to realize it is stopped for a few readings.

To be more prescriptive:
1. Let it sit after booting up for about a minute
2. Turn it on its side, hold it steady for 10s.
3. Rotate to a different side, hold it steady for 10s.
4. Flip it over, hold for 10s.
5. Back to original position.

That is 4 sides instead of 6 but should be enough. The ImuCal will tell you how well the unit is calibrated and give suggestions on how to fix errors (if there are any).

In the BEDS cage, this will be easier to roll it around. In the short term, I'm happy to show you over video.

Cheers,
Elecia
