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Mother Board Rev2 Wish List, high-to-low priority: 
1. Fix coin cell polarity & new (more reliable) coin cell holder.  

2. Internal monitoring of 3.3v coin cell voltage. 
3. Load test for Pack 1, Pack 2, reporting voltage at ~ 1mA load

4. Interface for Density Sensor? 

5. New mechanical and electrical interface for a new gen sensor board? 

6. Audio buzzer on Mother Board; Audio conformation of event triggering; Audio conformation of flowchart transitions 

7. Interface to self-tester: small motor to vibrate board? 
8. Interface to proximity sensor?
9. Bluetooth interface on the 2nd serial port,
with a power switch to turn it on/off.  We could leave it on for 24 hours during
"deploy" mode, then power cycle it at very low duty cycle.  Perhaps add a "recovery"
mode to again leave it on.  It allow us to make last minute changes during deployment and give us a way to recover data from a recovered can without opening the can.

Other improvements: 

1. Pressure sensor to avoid corrosion 

2. Revise mechanics 

