This directory contains the source code for the embedded BEDS controller – both the embedded code intended to be deployed, and test code for testing the embedded controller.
Contents
Project Files
BEDS.mcp - The Metrowerks Codewarrior project file to build the embedded BEDS software.  This project file has two targets:
· BEDS builds the software for the BEDS controller.
· BEDSProto builds it for the preliminary hand-wired prototype.
BEDSTest.mcp - The Metrowerks Codewarrior project file to build various test apps.  This project file has multiple targets:
· BEDSTeapot builds a version of the Invensense Teapot code that sends packets via the BEDS aux serial port, to talk to the Invensense Teapot Windows app.
· BEDSTeapotProto builds the teapot app for the hand-wired proto board.
· LPStop and LPStopProto build a simple app that can be used to measure the currentconsumption of the board in low-power sleep mode.
· decode builds a standalone program to decode BEDS event (.EVT) and watch (.WAT) files.  This builds as a standalone PicoDOS application
Directories containing source
src is the directory containing the 'C' source files for the BEDS application and tests.  It in turn has several subdirectories:
src/beds contains the code that directly implements the BEDS application.
[bookmark: _GoBack]src/umpl contains the platform-independent parts of the Invensense MotionApps stack
src/platform contains the platform-specific code from the Invensense MotionApps software stack, customized for the Persistor CF2
src/ZModem contains the source for ZModem file transfer
src/ekermit contains the source for Kermit file transfer
src/test contains code for test applications.

