Project Highlights

Benthic Event Detectors (BEDs) 901006
The BEDs project is progressing with inertial sensor selection and has narrowed the field to two possibilities. Work on the electrical and mechanical design has moved forward in anticipation of a preliminary design review in early 2012. Further requirements definition is continuing to refine what data will be transferred off the instrument to accurately measure and visualize the complex motion of a sediment debris flow.
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Figure � SEQ Figure \* ARABIC �1� – Initial Mechanical Design of BED. Sphere is 18” in diameter.








