
Note: “resp-kh.scp “ is the original script Craig O. gave to me to be modified and used as the resp.scp file that includes the sealing mechanism

Commands:
[bookmark: _GoBack]To open the valves use the “rempulse” command.
For chambers 1,2
rempulse open_1 45
 
For chambers 3,4
rempulse open_3 45       
rempulse close_3 45
to purge
rempulse open_1 240 
open the lure cap to purge

