Date: 12/28/22
Attendees: Carl Embry, Nelson Diaz, David Caress, Jenny Paduan, Eric Martin

Old Business

· Reviewed requirements and wishlist from concept phase
New Business

· System will be Class IV as currently specified due to new power and higher PRF of the laser.
· System will also get a little longer, approximately 29 in”
· Eric posits that the MHDL is a little outdated on MBARI’s uses, we could consider using the Subconn Ethernet and data series. DIL13 is a candidate cable.
· Changed requirement to mandate PPS, PTP as an upgrade path
· Presentation of the optical assembly
· Optical models of the bench also shown, spot sizes look good at close and far ranges (1-10m)
· Mock endcap fabricated, waiting for window bell to commence with under pressure testing of the rotating assembly
Action Items

· Validate changes on requirements
· MUST PPS, preferred PPS from preferred PTP (MBARI mostly)
· Change connector to Subconn DIL13 (MBARI verify, 3D check compatibility on voltage and current of new choice)
· Model in tilting sled (MBARI)
· Follow up on any institutional restrictions on Class IV lasers
· UPDATE: The LSO was contacted and MBARI see no issues aside from operations in the test tank for this power. We have controlled spaces if Class IV work needs to be done on site.
Next Meeting
· Jan 31st 2022, 10AM
