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Hans Thomas, Brett Hobson, David Caress, Eric Martin, Larry Bird


Among the issues to discuss are:
            1) What I saw at WHOI-DSL last week (Jon Howland's stereo camera rig).
            2) Camera choices
            3) Multibeam status
            4) Multibeam test plans
            5) Possible Postdoc joining the team later this year.
 
· Larry showed CAD drawings of the Ventana toolsled with multibeam arrays, cameras, INS, and housing. 
· Move the cameras back towards the center.  
· CBe able to place cameras either along or across the vehicle. 
· Strobes at all four corners. 
· Rough idea of the camera separation is 18 inches, but needs to be fully defined. 
· Put the INS as close as possible to the center to minimize lever arms to the sensors.
· Will get multibeam arrays within a couple of weeks.
· The Kearfott is still at Kearfott getting fixed
· Camera choices
· Reg Wilson says best you can do is get 12 bits dynamic range out of current camera sensors
· Can take multiple images with different settings (old style bracketing)
· Prosilicas have higher noise than specs would show. Steven McPhail at Southhampton is going to test Point Gray Grasshopper II camera. 
· All cameras use either a Sony or  a Kodak sensor.
· Can we get GigE to the surface?
· There are some media converters that should work on Ventana.
· What photo rate? 
· Figure ROV runs at 0.2 m/s. 
· Want to use a single trigger pulse, can have a trigger divisor on cameras and strobes. 
· Will need better than 50% overlap in pictures.
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