Ocean Imaging
Low Altitude Survey System (LASS)
Notes from MOB on R/V Carson December 2022


Friday 12/16/2022
USBL positions from Winfrog

Monday 12/19/2022
Terminal Screen
	OI_Deployments
	OI_Deployments/proc.cfg  -> Processes
GUI on TCU for Power Can control
Scripts
	Start control
	Start low power
	Procman_Sheriff
Navigate to folder Ventana_Date
		run ‘startlowpower’
		run ‘logthl’
		run ‘logthr’
Check everything through Procman_Sheriff
On Laptop,
	run ‘PC-DAS’
		Kearfott – ZDA/GPS data
		Paro – data
		Check Kearfott watchdog
[bookmark: _GoBack]run WISSL GUI
		PPS LED confirms good ZDA signal
		ZDA LED confirms good ZDA data
		Heads and CTD publication
	run Reson GUI
		Remote desktop
		Service – Diagnostic Screen
Strobes On
Oi_startall
	Cameras and strobes
	Begin logging data
Set Reson to Operate mode




