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Electrical
External trigger on Reson bad after plugging in the Oculus cable. (Wed 10/8)
DVL did external trigger. 

Tank testing next week.

Valve pack communication flaky (all 3 days)
    Had a temporary software fix.
    Valve pack electronics respin.

Mechanical
Reson receive head on backwards.

Norbit spacer to replace multiple washers.


Phins
Performed better on Wednesday. Why?
    Turn off Norbit? (interference?)
     Tuesday: glitches in position went away without DVL aiding.

Jumps in the ParoSci data

Is the DVL noisy?

Quaternions

GPS antenna on vehicle seemed to work
    Switch to RTK?

May need to recalibrate.

Do we need time tags on the depth messages?
USBL time tagging?
Reprocess with USBL aiding on (during calibration)

Modify DVL driver for compass.





Lidar
Negative voltage boot-up issue

Spin up/down time too long.
Spin up/down feature needs to be fixed.
Spin up/down number could be bolded.

Sriat data conversion still not working (time stamps).

Safety features for changing the optical power.

Playback angles are touchy in software. (sector view changes stop data logging)

Autoname changing feature needs some work (# of points in filename was wrong)
Subfolder changes were always manual.


Controls
Replace position viewer with DIAL.

UDP bridge to Ventana network modifications.




TCU
Incorporate HDMI splitters and keyboard/mouse extenders into TCU (or separate smaller stackable rack).

Clean up wiring in chassis box.



System
Capture Eric’s hand drawing of the control room components into OrCad LASS System Project.




