Instrument List
· Kearfott (w/Parasci mounted alongside)  
· Reson (Projector/Reciever) (120 degree width)
· LIDAR (90 degree width)
· Cameras and Lights
· TroniNav
· Sub-bottom profiler (non-tilting)
· Tilt Angle Sensor
Electronics  Housings
· LIDAR Electronics Can
· Power Can
· Reson Electronics Can
· Strobe Electronics Can
· Hydraulic Valve amplifier (non-tilting)
	
	Inside Width
	Inside Height

	Ricketts
	65 5/8”
	43”

	Subastian
	64 1/8”
	N/A

	Ventana
	62”
	40.75”
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120 Degree Range of Motion
100 -> -20 degrees
82 -> -35 degrees

Angular Speed
20 deg/sec per GPM.  	-> 1GPM Valve equals 6 seconds end to end.
-> 2GPM Valve equals 3 seconds end to end.

