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Pressure apparatus schematics from literature
1. Gross and Jaenicke 1994 Fig. 1B: T-path fluoro cell
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2. Mustafa, Moon and Hochachka 1971 Fig. 1: 5 cc 2-window cell with cleanout
NOTES: 
a. This is the cell Erik has.
b. It undergoes 12% expansion of path length (from 10 to 12 mm) at P > 2000 PSI.
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3. See Paladini and Weber 1981 for detailed drawings of a 2-4-window sealed-cuvette cell similar to what’s offered by ISS.
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