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The Self-Contained Plankton Imager (SCPI) prototype made a number of engineering test deployments in Monterey Bay throughout 2013. These tests successfully verified the operational capabilities of the SCPI system such as image quality, battery capacity, depth rating, and image & video storage. The results of these tests included both individual and time lapse images, and video clips. SCPI was tested on a variety of platforms including the ROV Ventana, a custom tripod, and full integration onto the Tethys class AUVs. As a result of the successful test deployments, two additional SCPI systems were built.

