Antarctica
Stacy Kim of MLML will be deploying two SCPI systems in Antarctica in late 2014 to help her study the benthic marine ecology of two locations near McMurdo Station. Both locations are located under 1 to 2 meters of ice and have never been photographed. The first location at Mystery peak is in 40 meters of water and both systems will be deployed for one month, taking an image every 20 minutes. The second location, between Tent Island and the Erebus Glacier Tongue, is in 200 meters of water. Both SCPI systems will again be deployed in this location, this time with extended primary lithium battery packs, allowing them to take an image every 20 minutes for 3 months.



F/V Donna Kathleen
A multi-organizational effort headed by Mary Gleason of The Nature Conservancy, Rick Starr of MLML, and Tim Maricich of the F/V Donna Kathleen are evaluating a SCPI system with the hopes of incorporating it into their instrumentation suite. They are interested in gathering density, size, and habitat-association data for rockfish and other demersal fish (eg. Lingcod). The initial thrust of their study is on the overfished species in fishery closure areas in federal water, specifically the Rockfish Conservation Area. In the future, similar surveys could be conducted in the state marine protected areas.

From Mary Gleason (5/28/2014):
Yes we are interested in getting density, size, and habitat-association data for rockfish and other demersal fish (eg. Lingcod) but with a particular focus in this study on the overfished species in fishery closure areas in federal waters (specifically the Rockfish Conservation Area).  For future applications we are interested in conducting similar surveys of nearshore rockfish species in the state marine protected areas.


Engineering Tests
[bookmark: _GoBack]Our initial deployments were focused on verifying that SCPI met all of our original functional requirements. SCPI was mounted onto ROV Ventana’s midwater tool sled and taken to its maximum operational depth of 300m. SCPI was also mounted to a simple horizontal bar and deployed to various sites in Monterey Bay including the swFOCE site at Hopkins Marine Station and an abandoned discharge pipe in Moss Landing.



