On Vicor Can 2, the trim pots were set as follows:
1. R19 = 5 Ohms, resulting +15V reading was +15.12V
2. R11 = 1 kOhm, resultant set point for circuit ~52V
[bookmark: _GoBack]These settings were based on what worked on one side of the bus need to be confirmed with original vicor can.
