65mm diameter 
59mm length
10 Amps RMS CRITICAL Future application

48V Peak Rover by wire
48V Peak Battery for future application; Do not know minimum voltage
1828 RPM under load
1.89 Nm Nominal Torque (possibly peak torque)

K064150-5Y1 appears to be golden motor based on 
· 10 Amps max
· 65mm Diameter 
· 96.8mm Length exceeds 59mm
· Peak Torque at 10 amps is 1.9 Nm
· Rated Torque at 10 Amps (7 amps RMS) only 1.4 Nm
K089075-5Y1 possible golden motor based on Torque continuous
· 10 Amps Max
· 89 mm Diameter over exceeds 65mm
· 25mm Length below dimension requirement
· Peak Torque at 10 amps is 2 Nm
· Rated Torque at 10 amps at 2Nm

