Configuration of P8
	P8 Pin
	Proc
	BB Signal
	Mode0 Name
	GN Signal
	Type
	BB Mode
	Mux Value

	1
	GND
	GND
	 
	GND
	Gnd
	N/A
	 

	2
	GND
	GND
	 
	GND
	Gnd
	N/A
	 

	3
	R9
	GPIO1_6
	gpmc_ad6
	NODE_4_OFF
	Digital Out
	7
	7

	4
	T9
	GPIO1_7
	gpmc_ad7
	NODE_4_ON
	Digital Out
	7
	7

	5
	R8
	GPIO1_2
	gpmc_ad2
	NODE_3_OFF
	Digital Out
	7
	7

	6
	T8
	GPIO1_3
	gpmc_ad3
	 
	 
	 
	 

	7
	R7
	TIMER4
	gpmc_advn_ale
	BB_R7
	Unused
	2
	 

	8
	T7
	TIMER7
	gpmc_oen_ren
	BB_T7
	Unused
	2
	 

	9
	T6
	TIMER5
	gpmc_be0n_cle
	BB_T6
	Unused
	2
	 

	10
	U6
	TIMER6
	gpmc_wen
	BB_U6
	Unused
	2
	 

	11
	R12
	GPIO1_13
	gpmc_ad13
	NODE_2_OFF
	Digital Out
	7
	7

	12
	T12
	GPIO1_12
	gpmc_ad12
	NODE_2_ON
	Digital Out
	7
	7

	13
	T10
	EHRPWM2B
	gpmc_ad9
	BB_T10
	Unused
	7 (gpio0_23)
	 

	14
	T11
	GPIO0_26
	gpmc_ad10
	EEPROM_WP1
	Digital Out
	7
	7

	15
	U13
	GPIO1_15
	gpmc_ad15
	NODE_1_OFF
	Digital Out
	7
	7

	16
	V13
	GPIO1_14
	gpmc_ad14
	NODE_1_ON
	Digital Out
	7
	7

	17
	U12
	GPIO0_27
	gpmc_ad11
	EEPROM_WP2
	Digital Out
	7
	7

	18
	V12
	GPIO2_1
	gpmc_clk_mux0
	EEPROM_WP3
	Digital Out
	7
	7

	19
	U10
	EHRPWM2A
	gpmc_ad8
	BB_U10
	Unused
	7(gpio0_22)
	 

	20
	V9
	GPIO1_31
	gpmc_csn2
	ENVR_ALARM
	Digital In
	7
	39

	21
	U9
	GPIO1_30
	gpmc_csn1
	EEPROM_WP4
	Digital Out
	7
	7

	22
	V8
	GPIO1_5
	gpmc_ad5
	H2O_ALARM
	Digital In
	7
	39

	23
	U8
	GPIO1_4
	gpmc_ad4
	48V_RET_GF
	Digital Out
	7
	7

	24
	V7
	GPIO1_1
	gpmc_ad1
	TEST_RET_GF
	Digital Out
	7
	7

	25
	U7
	GPIO1_0
	gpmc_ad0
	48V_GF
	Digital Out
	7
	7

	26
	V6
	GPIO1_29
	gpmc_csn0
	TEST_GF
	Digital Out
	7
	7

	27
	U5
	GPIO2_22
	lcd_vsync
	NODE_1_STATE
	Digital In
	7
	39

	28
	V5
	GPIO2_24
	lcd_pclk
	NODE_3_STATE
	Digital In
	7
	39

	29
	R5
	GPIO2_23
	ldc_hsync
	NODE_2_STATE
	Digital In
	7
	39

	30
	R6
	GPIO2_25
	lcd_ac_bias_en
	NODE_4_STATE
	Digital In
	7
	39

	31
	V4
	UART5_CTSN
	lcd_data14
	BB_V4
	BT/Unused
	7
	7

	32
	T5
	UART5_RTSN
	lcd_data15
	BB_T5
	BT/Unused
	7
	7

	33
	V3
	UART4_RTSN
	lcd_data13
	BB_V3
	BT/Unused
	7
	7

	34
	U4
	UART3_RTSN
	lcd_data11
	BB_U4
	BT/Unused
	7
	7

	35
	V2
	UART4_CTSN
	lcd_data12
	BB_V2
	BT/Unused
	7
	7

	36
	U3
	UART3_CTSN
	lcd_data10
	BB_U3
	BT/Unused
	7
	7

	37
	U1
	UART5_TXD
	lcd_data8
	UART5_TTL_TXD
	BT/Unused
	4
	 

	38
	U2
	UART5_RXD
	lcd_data9
	UART5_TTL_RXD
	BT/Unused
	4
	 

	39
	T3
	GPIO2_12
	lcd_data6
	BB_T3
	BT/Unused
	7
	7

	40
	T4
	GPIO2_13
	lcd_data7
	BB_T4
	BT/Unused
	7
	7

	41
	T1
	GPIO2_10
	lcd_data4
	BB_T1 
	BT/Unused
	7
	7

	42
	T2
	GPIO2_11
	lcd_data5
	BB_T2
	BT/Unused
	7
	7

	43
	R3
	GPIO2_8
	lcd_data2
	BB_R3
	BT/Unused
	7
	7

	44
	R4
	GPIO2_9
	lcd_data3
	BB_R4
	BT/Unused
	7
	7

	45
	R1 
	GPIO2_6
	lcd_data0
	BB_R1
	BT/Unused
	7
	7

	46
	R2
	GPIO2_7
	lcd_data1
	[bookmark: _GoBack]BB_R2
	BT/Unused
	7
	7


Configuration of P9
	P9 Pin
	Proc
	BB Signal
	Mode0 Name
	GN Signal
	Type
	BB Mode
	Mux Value

	1
	GND
	GND
	 
	GND
	Gnd
	N/A
	 

	2
	GND
	GND
	 
	GND
	Gnd
	N/A
	 

	3
	3.3VEXP
	3.3VEXP
	 
	3.3V
	Power
	N/A
	 

	4
	3.3VEXP
	3.3VEXP
	 
	3.3V
	Power
	N/A
	 

	5
	VDD_5V
	VDD_5V
	 
	5V_BB
	Power
	N/A
	 

	6
	VDD_5V
	VDD_5V
	 
	5V_BB
	Power
	N/A
	 

	7
	SYS_5V
	SYS_5V
	 
	5V 
	Power
	N/A
	 

	8
	SYS_5V
	SYS_5V
	 
	5V
	Power
	N/A
	 

	9
	 
	PWR_BUT*
	 
	PWR_BUT*
	Special
	N/A
	 

	10
	A10
	SYS_RESETn
	RESET_OUT
	SYS_RESETn
	Special
	0
	 

	11
	T17
	UART4_RXD
	gpmc_wait0
	UART4_TTL_RXD
	Serial
	6
	 

	12
	U18
	GPIO1_28
	gpmc_be1n
	NODE_3_ON
	Digital Out
	7
	7

	13
	U17
	UART4_TXD
	gpmc_wpn
	UART4_TTL_TXD
	Serial
	6
	 

	14
	U14
	EHRPWM1A
	gpmc_a2
	BB_U14
	Unused
	7(gpio1_18)
	 

	15
	R13
	GPIO1_16
	gpmc_a0
	BB_R13
	Unused
	7
	 

	16
	T14
	EHRPWM1B
	gpmc_a3
	BB_T14
	Unused
	7(gpio1_19)
	 

	17
	A16
	I2C1_SCL
	spi0_cs0
	BB_A16
	Unused
	7(gpio0_5)
	 

	18
	B16
	I2C1_SDA
	spi0_d1
	BB_B16
	Unused
	7(gpio0_4)
	 

	19
	D17
	I2C2_SCL
	uart1_rtsn
	I2C2_SCL
	I2C Bus
	3
	 

	20
	D18
	I2C2_SDA
	uart1_ctsn
	I2C2_SDA
	I2C Bus
	3
	 

	21
	B17
	UART2_TXD
	spi0_d0
	UART2_TTL_TXD
	Serial
	1
	 

	22
	A17
	UART2_RXD
	spi0_sclk
	UART2_TTL_RXD
	Serial
	1
	 

	23
	V14
	GPIO1_17
	gpmc_a1
	BB_V14
	Unused
	7
	 

	24
	D15
	UART1_TXD
	uart1_txd
	UART1_TTL_TXD
	Serial
	0
	 

	25
	A14
	GPIO3_21
	mcasp0_ahclkx
	BB_A14
	Unused
	7
	 

	26
	D16
	UART1_RXD
	uart1_rxd
	UART1_TTL_RXD
	Serial
	0
	 

	27
	C13
	GPIO3_19
	mcasp0_fsr
	BB_C13
	Unused
	7
	 

	28
	C12
	SPI1_CS0
	uart1_rxd
	SPI1_CS0
	SPI Bus
	3
	 

	29
	B13
	SPI1_DO
	mcasp0_fsx
	SPI1_MOSI
	SPI Bus
	3
	 

	30
	D12
	SPI1_DI
	mcasp0_axr0
	SPI1_MISO
	SPI Bus
	3
	 

	31
	A13
	SPI1_SCLK
	mcasp0_aclkx
	SPI1_SCLK
	SPI Bus
	3
	 

	32
	1.8VREF
	1.8V_REF
	 
	1.8V_REF
	Volt Ref
	N/A
	 

	33
	C8
	AIN4
	 
	GF_CURR
	Analog In
	N/A
	 

	34
	GNDADC
	GNDA_ADC
	 
	GNDA_ADC
	Analog Gnd
	N/A
	 

	35
	A5
	AIN6
	 
	48V_CURR
	Analog In
	N/A
	 

	36
	A5
	AIN5
	 
	48V_VOLT
	Analog In
	N/A
	 

	37
	B7
	AIN2
	 
	NODE_3_CURR
	Analog In
	N/A
	 

	38
	A7
	AIN3
	 
	NODE_4_CURR
	Analog In
	N/A
	 

	39
	B6
	AIN0
	 
	NODE_1_CURR
	Analog In
	N/A
	 

	40
	C7
	AIN1
	 
	NODE_2_CURR
	Analog In
	N/A
	 

	41
	D14
	CLKOUT2
	xdma_event_intr1
	BB_D14
	Unused
	3
	 

	42
	C18
	GPIO0_7
	eCAP0_in_PWM0_out
	SPI1_CS1
	SPI Bus
	2
	 

	43
	GND
	GND
	 
	GND
	Gnd
	N/A
	 

	44
	GND
	GND
	 
	GND
	Gnd
	N/A
	 

	45
	GND
	GND
	 
	GND
	Gnd
	N/A
	 

	46
	GND
	GND
	 
	GND
	Gnd
	N/A
	 



