Pin Out Configuration - data cables  4/25/07

	 
	

	PIL-8-FS
	PIL-8-MP

	1
	1 cat5 blue/white

	2
	2 cat5 blue

	3
	3 red conductor (16AWG)

	4
	4 purple conductor (16AWG)

	5
	5 cat5 yellow/white

	6
	6 cat5 yellow

	7
	7 cat5 green/white

	8
	8 cat5 green
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