FOCE Chassis Power Supply Engineering Change Orders


A - SPI2 MISO line modification

	Pull U7-1 leg off of pad.
	
	Tie U7-1 raised leg to U4-3.

	











