FOCE Chassis Power Supply Board Software Commands



GetFanState
	RB6 - Digital In
	High (1) = Fan Off
	Low (0) = Fan On

SetFanState
	RB5 - Digital Out
	High (1) = Turns fans on
	Low (0) = Turns fans off 

SPI_1_CS
	RA0 [TEMP_0_CS] - 0
	RA1 [TEMP_1_CS] - 1
	RB8 [TEMP_2_CS] - 2
	RB4 [ADC_CS] - 3
	High (1) = No SPI device selected
	Low (0) = SPI device [0, 1, 2, or 3] selected	
	
Beta_Sync
	RA4 - Digital Out
	Oscillates at xx Hz




