


FOCE Chassis Software Architecture



FOCE Chassis CPU Board

Board Features

	1. Board level 1M EEPROM IC
	2. Board level SD card
	3. XPort Ethernet interface
	4. Monitors for daughterboard interrupts
	5. Generates bus level dig out signals (x2)
	6. Monitors for bus level dig in signals (x2)
	7. Generates dedicated power supply dig out signals (x3)
	8. Master of bus level SPI communications
	9. Generates board specific addresses for dig out and CS* signals



