FOCE Instrument Chassis Environmental Board ECO List

Board: 10020577 Rev A



A: 	SPI bus #1 CS needs a pullup resistor.
	Add a 10k pullup resistor to U4-11. A 1206 sized resistor tied between U4-11 and U4-14 fits 	perfectly if the resistor is mounted ontop of the IC.
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B: 	SPI bus #1 has MISO and MOSI reversed going into the PIC. 
	Lift U6-2 and U6-6 legs.
	Solder wire from U6-2 raised leg to U6-6 pad.
	Solder wire from U6-2 pad to U6-6 raised leg.
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