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Existing DNS Names
	IP Address
	DNS Name
	Function

	134.89.91.1
	
	Router

	134.89.91.2
	kelpbed
	Pumphouse Linux box

	134.89.91.3
	swfoce-serial
	Was QuickFOCE Digi terminal server, now unused

	134.89.91.4
	swfoce2
	Was Digi terminal server in pumphouse

	134.89.91.5
	swfoce3
	Pumphouse OE Converter

	134.89.91.6
	
	Deployed (wet) OE Converter



Proposal
IP Blocks:
	134.89.91.1 – 31
	Infrastructure & pump house

	134.89.91.32 - 63
	swFOCE1

	134.89.91.64 – 95
	swFOCE2

	134.89.91.96 - 254
	Unused



[bookmark: _GoBack]Proposed changes for DNS names.  Note all are on subnet swfoce.mbari.org.  That’s why they no longer carry the “sw” prefixes in the DNS name themselves.
	IP Address
	DNS Name
	Function

	134.89.91.1
	
	Router

	134.89.91.2
	kelpbed
	Pumphouse Linux box

	134.89.91.3
	serial1
	Was QuickFOCE Digi terminal server, now unused

	134.89.91.4
	serial2
	Was Digi terminal server in pumphouse

	134.89.91.5
	oe1
	Pumphouse OE Converter

	134.89.91.6
	oe2
	Deployed (wet) OE Converter

	134.89.91.7
	cn
	Central Node matchport serial server

	
	
	

	134.89.91.32
	gw1
	Gateway node 1

	134.89.91.33
	gw1serial
	Digi serial server in gateway 1

	134.89.91.34
	gw1camera
	IP Camera on gateway 1

	
	
	

	134.89.91.64
	gw2
	Gateway node 2

	134.89.91.65
	gw2serial
	Digi serial server in gateway 2

	134.89.91.66
	gw2camera
	IP Camera on gateway 2



