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Project Title:

Particle characterization technology for autonomous platforms
1) ABSTRACT (new projects only)
   [Paste abstract here]   

2) PROPOSAL
a) New Projects
Statement of the problem, why it is important
   [Click here to enter text]   
How does it relate/contribute to MBARI’s mission and strategic plan?
   [Click here to enter text]   
How does it relate/contribute to the Packard Foundation’s Ocean Visions Grantmaking policies? (See http://mww.mbari.org/oed/OED_Documents3.htm#Packard for documents.)
   [Click here to enter text]   
Approach to the problem
   [Click here to enter text]   
Publications (from other projects over the last 5 years)

   [Click here to enter text]   
b) Continuing Projects

If the proposed project includes multiple individual projects, please list each of these projects as a subheading in the proposal. For each subheading, please address the following:

Current status of project and results to date
All of our work is documented on the MBARI Confluence wiki at https://oceana.mbari.org/confluence/display/CytometerTech/Home
We have reviewed and compared characteristics and capabilities of existing oceanographic cytometers that have been or could potentially be integrated with Dorado or LRAUV [table], based on size, complexity and power requirements. Our investigation has clarified that flow cytometers are most appropriate to small (< 10 micron) spherical particles, while imaging cytometers are best suited to larger, non-spherical particles with more complex morphologies. Some cytometers such as Imaging Flow CytoBot, FlowCam and CytoSub include both pulse and imaging capabilities.  
We have reviewed some techniques beyond flow and imaging cytometry that are at various maturity stages, including Coulter counters, holographic imagers, bulk optical techniques, mass spectrometric cytometry and microfluidic cytometry. We are arranging these in a matrix to evaluate applicability and potential adaptability to AUVs. 

In addition to reviewing the 2010 CANON Sampling workshop report, we conducted interviews with Worden, Chavez, and Ryan to better understand MBARI science requirements. We held discussions with Jared Swalwell for updates on SeaFlow and SeaLabel development plans. Bellingham and Chavez initiated discussion with Fluid Imaging, and may procure a FlowCam instrument this year for evaluation during CANON. Chavez plans to request CANON use of a CytoBuoy instrument owned by Dick Dugdale's lab at San Francisco State University.  We hope to invite a guest seminar speaker this year - possibly Heidi Sosik or Jared Swalwell.  We held a telecon with Holomic LLC, who are designing low-cost cytometric blood counters for developing world medical use; we learned that this technology is still in early development stage, and it is not clear if it can be adapted to oceanographic use.
We have learned that cytometers are somewhat limited in the range of particles that can be measured, especially flow cytometers, and we have not identified a specific cytometer or technology that can measure particles across the entire range of interest to CANON scientists (0.5 microns to millimeters in size). Given the fluidics design of many of these instruments, it's now clear that cytometer integration times of many minutes may be needed to acquire statistically significant cell counts, depending on number density of the target organism. These long integration times are problematic on a moving AUV that may move into completely different populations of organisms within a time span of seconds.  Of these AUV-compatible instruments, we've determined that only SeaFlow has the required sensitivity (~0.5 micron) to address research interests of the Worden lab, while several of the others could be useful to Chavez' work. 
This year (2013) we plan to build a fluorescence microscopy test-bed as a means to test concepts and gain invaluable experience in building instrumentation that is very relevant to CANON goals. Klimov is currently designing test bed optics and other hardware; we plan to demonstrate the test bed at the end of 2013, with exploration of analysis algorithms planned for 2014. Note that this lab test-bed does not indicate readiness to build an actual sea-going instrument; rather it will give us better understanding of cytometry principles and technical approaches, and develops very valuable experience at MBARI. [DENIS, MORE DETAIL HERE PLEASE]. 
Moreover as this and other instrumentation projects have progressed in 2013, we now increasingly understand that the suite of in situ instruments currently in use at MBARI, even on the very well-equipped Dorado vehicle, do not yet provide an integrated characterization of particles and organisms across the size scales of interest. In many cases users do not fully understand the capabilities and limitations of these instruments, and in some cases the instruments are not sufficiently calibrated. Thus Bellingham is spinning off a project in his lab that will characterize the capabilities and characteristics of those instruments, utilizing standard samples that may include monocultures, "wild" samples and calibration beads. In addition that project will examine data processing algorithms in more detail.  Our cytometer feasibility project will have access to those standard samples for testing Klimov's fluorescent microscope test-bed, and we also propose to explore approaches to analysis of the images produced by that instrument. Thus we expect considerable synergy between these two projects.

Significant changes from previous project proposal 

Publications based on the results of this project only
   [Click here to enter text]   
c) New and Continuing Projects: Plans for 2014
Research Activities
None
Engineering/technology development

Our goal is to identify technology that would enable in situ cytometry aboard an AUV. Image processing software is required to analyze the data generated by imaging cytometers. For small semi-spherical particles, it is straightforward to measure dimensions and fluorescent intensity, which might be sufficient to at least narrow the range of potential target IDs. More sophisticated software is required for morphologically complex particles. Image analysis software (e.g. MBARI's AVED or Fluid Imaging's "Visual Spreadsheet") generally requires that the software be "trained" by a human to recognize particular targets and needs significant CPU power that is not currently available in AUVs. Moreover it is not clear how accurate the software is in identifying CANON targets of interest.  

· Measure how accurately CANON-relevant species can be identified by image-processing software such as AVED or Visual Spreadsheet. We will utilize standard samples provided by Bellingham's lab project for this work. 

· Discuss candidate in situ processing approaches and hardware being explored by the HIPP project within CANON;  Thom Maughan has been researching hardware that could potentially host AVED software, a nd we believe that both projects could benefit from discussions.

Alex Worden will be available in an advisory role for up to 12 hours next year. 

As noted earlier, our project is closely related to Bellingham's plans to characterize the current suite of AUV instrumentation, and there is extensive mutual interest in the progress of both projects. 

DENIS TEXT HERE.
Field programs (detail ship requirements/deployments/diver requirements)
None
Specific deliverables
· Fluorescent microscope test-bed

· Final Report

Milestones (see personnel classification list)
   [Click here to enter text]   
	2014 Project Start Date: 
MM/DD/2014
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Budget justification
   [Click here to enter text]   
Project team
Francisco Chavez - Lead scientist

Denis Klimov - Lead engineer
Tom O'Reilly - Project manager
Project lab space
Lab space in the B232 is well equipped with electrical and opto-electronic test equipment and work space; and should be sufficient for proposed activity. Any LRAUV-specific test can be performed in the LRAUV lab. 
Data availability outside project team, uniqueness

No data outside project team will be made available. 

Export Regulation
Does the project team anticipate any foreign collaborations or international travel? If so, please identify collaborators by name, institution, and country.

No.
Does the project team plan or anticipate export controlled purchases, shipments, or transfers of items (e.g., research instruments, proprietary data, hand-carried tools or samples) outside the U.S. temporarily or permanently? If yes, please identify country or countries and indicate whether these items will remain under MBARI control while abroad or controlled by others. Will the items be exported to more than one country? Please include foreign collaborator information as described above.

No.
Monterey Bay National Marine Sanctuary SESAs (General map)
Projects will need to indicate whether or not work will be conducted within one of the Monterey Bay National Marine Sanctuary's Ecologically Significant Areas (SESAs). An interactive map can be found on the Sanctuary's SIMoN webpages at http://sanctuarysimon.org/maps/sesa/. (Note: It may take a moment for the page to load, so please be patient.) To determine if your work will occur in a SESA, specific coordinates can be entered using the locator function (click on the red "target" button in the toolbar at the top of the map). If your work will be conducted in one of these areas, please indicate which area, by number. 

None.
Risk matrix (development and infrastructure projects only)
	
	Technical Risk
	Organizational Risk
	Tech Transfer Risk
	Labor Estimate Risk

	High
	
	
	
	

	Medium
	
	
	
	

	Low
	
	
	
	


� Development and infrastructure projects must complete the risk matrix (see item #5 at the end of the proposal form).


� Not all projects will require all four titles to be filled in. Please indicate individuals only for those titles that are appropriate for your project. 


� This number should be the same number you entered on the resource requests for this particular resource.
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