
· OTG IOIO Board 
· 16 inputs 0-3.3V  3mV resolution 
· Output 3.3V, 5V
· Digital I/O 3.3V logic 46 pins 
· Control of Light source 

Mother board: 
· Input 12-15 V = > Vin power to OTG IOIO board
· [bookmark: _GoBack]GPIO indicators: LED surface mount, output to scope 


Tom tried: analog input, UART


