3/22/2016 4-Deep visit/ demo. John Sampson (4-Deep), Hill Yuan (Senior Technical Adviser, Bosma, Guangzhou Bosma Corp), Robert Ji (Director/ Sales and Marketing, Bosma USA Inc)
10:30 arrival/ set up in B232
11:00 Klimov got beach water with tray  
11:10 Thom Maughan – taking harbor water sample with Robert Ji
11:15 Shannon Johnson has Micromonas sample / 10 mL cuvette 
11:30 Running octopus software with beach water, harbor water, and Micromonas mix with fresh water 
11:45 Heike Schmitz, Kurt Kiesow, Kakani Katija came
12:00 running Swordfish with Micromonas 
Kakani: need volume and even faster rate to pre-screen sample before light sheet measurements. . 
12:30 clean chamber, pump beach water from 11:10
Kurt: imaging volume? 
John: couple of mL. Volume looks like truncated pyramid 
Kurt: long and thin object (cell), oriented towards viewer. Can you measure its length?  
John:  tricky. Processing power is limiting here. 2 GB per hologram reconstructed – so one is reconstructed at the time. 
Kurt: 2 different wavelengths? Better resolution?  
John: say green and blue, then could cut 1.75 um resolution down to sub um
13:00 lunch
[bookmark: _GoBack]14:00: software installation on the lab computers. 
  


