	[bookmark: _GoBack]Function
	WGMS Tab
	Pwr Domain
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	Port #

	[bookmark: OLE_LINK1]Weather Station
	AMPS Output
	1
	4
	1

	Sensor Port 3 (S3)
	AMPS Output
	1
	4
	2

	Light Bar
	AMPS Output
	1
	4
	3

	Water Speed Sensor
	AMPS Output
	1
	4
	5

	Cell Modem
	AMPS Output
	1
	4
	6

	Radar Reflector
	AMPS Output
	1
	5
	1

	Float Recovery Device
	AMPS Output
	1
	5
	2

	Ethernet Switch
	AMPS Output
	1
	5
	3

	MAS Power (Surfer config only)
	AMPS Output
	1
	5
	6

	48V Surfer Streamer (Surfer config only)
	AMPS Output
	1
	5
	7

	High Voltage Port (HV)
	AMPS Output
	1
	5
	8

	Sensor Port 2 (S2)
	AMPS Output
	1
	7
	1

	Sensor Port 1 (S1)
	AMPS Output
	1
	7
	2

	AIS
	AMPS Output
	1
	7
	4

	Iridium Modem
	AMPS Output
	1
	32
	1

	Ublox GPS Module
	AMPS Output
	1
	32
	2

	Vehicle Management Computer
	AMPS Output
	1
	32
	3

	Thruster
	AMPS Output
	2
	1
	1

	
	
	
	
	

	Expansion Port 1 (G1), [Vcons, Vprod]
	AMPS Bridge
	1
	11
	1,2

	Expansion Port 2 (G2), [Vcons, Vprod]
	AMPS Bridge
	1
	12
	1,2

	Expansion Port 3 (G3), [Vcons, Vprod]
	AMPS Bridge
	1
	8
	1,2

	Umbilical Expansion Port (U1), Vcons
	AMPS Bridge
	1
	15
	1

	Debug Expansion Port (D1) [Vcons, Vprod]
	AMPS Bridge
	1
	14
	1,2

	Sub Expansion Port, Vcons
	AMPS Bridge
	2
	0
	5

	
	
	
	
	

	Fore Solar Panel
	AMPS Solar Input
	1
	9
	1

	Mid Solar Panel
	AMPS Solar Input
	1
	10
	1

	Aft Solar Panel
	AMPS Solar Input
	1
	10
	2
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