Missing several libraries and executables from Hotspot SMC - unable to run autoranging.py
Manually run (nohup) 800 meter watch circle centered at approximate Rover location, while runing ranging.py at 30 sec interval.
When Iridium modem hangs up unexpectedly while tailing nohup.out, have difficulty reconnecting - baud seems messed up- had to reboot SMC after circle completion

Got many good ranges - Ivan analyzing…

Working with Rich Henthorn to get rover status. Enabled Rover modem’s power bit with AT$X3,1 - but no messages from Rover. Issued ‘connect’ on rover’s acoustic channel twice a minute for 15 minutes, but no response.