Feb 27th, 2019 DeepPIV Improvement Meeting
In attendance: Randy, Mike B, DJ, Jon, Kakani, Joost, Alana, Marko

· Current proposed design changes:
· Move handle to middle position; both ROV teams in agreement
· Remove comp, move pump
· Modification of existing assembly rather than new build
· [bookmark: _GoBack]Pilots happy with 90 degree remote head cable design
· Sponge osculum view
· Discussion based on image below from (most recent) benthic dive on Feb 19th 2019 with DeepPIV 3 on Ventana
· Same orientation should be possible after modifications if manipulator moves are done with care
· Sag in system visible in image; investigate source when rebuilding system
· Could angle handle to accommodate range of motion
· Implementation of focal 914 fiber comms not deemed necessary at this time. It will not improve mob
· New T4 manipulator might be useful for the tall ocean imaging sled in the near future
· Hydraulic ram design
· Design looks good to all present
· Won’t need ram on Ventana for 2019
· Might conflict with samplers / swing arm to some extent
· Swing arm needs to be high to swing above laser (or similar solution)
· Action items
· Marko to move pump, remove comp, move handle, reassemble. Joost will help. March is good window of opportunity, start after board tour March 5th
· Check source of sag and rigidity of top handle.
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