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The connectors that we have used are Souriau and Bulgin.  We used the Souriau connectors on the transducers because they seem to be the best quality of the lower cost plastic connectors.  The Bulgins are solid, and they make that battery connector with large enough contacts to make sure that we're not creating pinch points at the bulkheads and dropping too much voltage.

I've attached a spreadsheet that lists all the connectors and specific part numbers, so you can look things up as you see fit.  I've also put the Souriau and Bulgin catalogs in Kelly's tempbox \kbb (I didn't see your tempbox...?).  In this email, I've put links to the connector series overview for each type.

Transducer cable connectors are the Souriau UTS Series:
IP68/69K
UV Resistant
Bayonet style coupler
We're using #20AWG contacts
http://usa.esterline-connection-technologies.com/en-en/products/connectors/circular-connectors/uts-series-plastic-waterproof-ip6869k-connector
https://ipaper.ipapercms.dk/SOURIAU/UTSSeriesUS2015/

Battery connectors are the Bulgin Buccaneer 900 Series:
IP68/69K
32A/600V rated
http://www.bulgin.com/products/circular-power-connectors/900-series.html
http://www.bulgin.com/media/bulgin/data/900%20Series.pdf
  
Grounding wire connectors are the Bulgin Mini Series:
IP68
http://www.bulgin.com/products/circular-power-connectors/mini-series.html
http://www.bulgin.com/media/bulgin/data/Mini_power.pdf

Ethernet connectors are the Bulgin Standard Series Ethernet:
IP68
CAT5e
http://www.bulgin.com/products/circular-data-connectors/standard-rj45-ethernet.html
http://www.bulgin.com/media/bulgin/data/Standard_ethernet.pdf


