Benthic Observation Survey System (BOSS) Maintenance
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Already covered in Lander Recovery section
Inspecting for lander damage upon recovery
Rinsing off lander/tether upon recovery
Squirting distilled water on camera ports
Confirming cables are properly secured to lander with zip ties
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