MBARI MXD 4K Camera

Record of topside optical uplink power readings measured at ST connector at rack mount box. Note minimum allowable optical power on 1310 nm is around ~-14 dBm.

Date		Optical Power				Notes__________________
 1/28/2022	Focal link 	1550 nm__-7.63 dBm_	               camera re-installed after
[bookmark: _GoBack]_________	12G 4k video 	1310 nm__- 5.83 dBm_                   optical measurements

Date		Optical Power				Notes__________________
		Focal link 	1550 nm___________	               
_________	12G 4k video 	1310 nm___________                   

Date		Optical Power				Notes__________________
		Focal link 	1550 nm___________	               
_________	12G 4k video 	1310 nm___________                  

Date		Optical Power				Notes__________________
		Focal link 	1550 nm___________	               
_________	12G 4k video 	1310 nm___________  






Mrc 1/28/2022
