(module IND_100M-D_TDK (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value IND_100M-D_TDK (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at 0 0) (layer F.SilkS))
  (fp_text user "*" (at 0 0) (layer F.Fab))
  (fp_text user "0.193in/4.902mm" (at 5.4991 0) (layer Cmts.User))
  (fp_text user "0.528in/13.411mm" (at 0 9.4996) (layer Cmts.User))
  (fp_text user "0.339in/8.6mm" (at 0 -9.4996) (layer Cmts.User))
  (pad 1 smd rect (at -5.5028 0) (size 2.4056 4.9022) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 5.5028 0) (size 2.4056 4.9022) (layers F.Cu F.Paste F.Mask))
)
