(module IND_A-4R7M (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value IND_A-4R7M (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at 0 0) (layer F.SilkS))
  (fp_text user "*" (at 0 0) (layer F.Fab))
  (fp_text user "0.197in/5.004mm" (at 5.5499 0) (layer Cmts.User))
  (fp_text user "0.559in/14.199mm" (at 0 9.4488) (layer Cmts.User))
  (fp_text user "0.315in/8.001mm" (at 0 -9.4488) (layer Cmts.User))
  (pad 1 smd rect (at -5.5499 0) (size 3.0988 5.0038) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 5.5499 0) (size 3.0988 5.0038) (layers F.Cu F.Paste F.Mask))
)
