(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "ADP7142ACPZN-R7:ADP7142ACPZN-R7" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -10.16 13.462 0))
      (property "Value" "ADP7142ACPZN-R7" (at -10.16 -15.24 0))
      (property "Footprint" "SON65P200X200X65-7N" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "PARTREV" "E" (at 0 0 0))
      (property "MF" "Analog Devices" (at 0 0 0))
      (property "SNAPEDA_PACKAGE_ID" "19057" (at 0 0 0))
      (property "STANDARD" "IPC-7351B" (at 0 0 0))
      (symbol "ADP7142ACPZN-R7_0_0"
        (rectangle (start -10.16 -12.7) (end 10.16 12.7)
          (fill (type background))
        )
        (pin output line (at 15.24 7.62 180) (length 5.08)
          (name "VOUT")
          (number "1")
        )
        (pin input line (at 15.24 2.54 180) (length 5.08)
          (name "SENSE/ADJ")
          (number "2")
        )
        (pin power_in line (at 15.24 -7.62 180) (length 5.08)
          (name "GND")
          (number "3")
        )
        (pin input line (at -15.24 2.54 0) (length 5.08)
          (name "EN")
          (number "4")
        )
        (pin passive line (at 15.24 -2.54 180) (length 5.08)
          (name "SS")
          (number "5")
        )
        (pin input line (at -15.24 7.62 0) (length 5.08)
          (name "VIN")
          (number "6")
        )
        (pin power_in line (at 15.24 -10.16 180) (length 5.08)
          (name "EP")
          (number "7")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.635 2.54 0))
      (property "Value" "C" (at 0.635 -2.54 0))
      (property "Footprint" "" (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (at 0 0 0))
      (property "ki_fp_filters" "C_*" (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (at 0 2.54 0))
      (property "Value" "LED" (at 0 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "LED diode" (at 0 0 0))
      (property "ki_description" "Light emitting diode" (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "R" (at 0 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
  )
  (junction (at 170.18 137.16) (diameter 0) (color 0 0 0 0))
  (junction (at 177.8 137.16) (diameter 0) (color 0 0 0 0))
  (junction (at 201.93 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 137.16 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 173.99 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 124.46 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 184.15 137.16) (diameter 0) (color 0 0 0 0))
  (junction (at 124.46 137.16) (diameter 0) (color 0 0 0 0))
  (junction (at 184.15 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 173.99 137.16) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 170.18 111.76) (xy 173.99 111.76)))
  (wire (pts (xy 137.16 106.68) (xy 124.46 106.68)))
  (wire (pts (xy 201.93 106.68) (xy 201.93 114.3)))
  (wire (pts (xy 110.49 106.68) (xy 124.46 106.68)))
  (wire (pts (xy 177.8 116.84) (xy 177.8 121.92)))
  (wire (pts (xy 170.18 124.46) (xy 170.18 137.16)))
  (wire (pts (xy 184.15 106.68) (xy 201.93 106.68)))
  (wire (pts (xy 201.93 106.68) (xy 210.82 106.68)))
  (wire (pts (xy 184.15 137.16) (xy 201.93 137.16)))
  (wire (pts (xy 111.76 137.16) (xy 124.46 137.16)))
  (wire (pts (xy 177.8 137.16) (xy 184.15 137.16)))
  (wire (pts (xy 201.93 130.81) (xy 201.93 137.16)))
  (wire (pts (xy 137.16 111.76) (xy 137.16 106.68)))
  (wire (pts (xy 124.46 118.11) (xy 124.46 137.16)))
  (wire (pts (xy 173.99 106.68) (xy 184.15 106.68)))
  (wire (pts (xy 170.18 116.84) (xy 177.8 116.84)))
  (wire (pts (xy 170.18 121.92) (xy 173.99 121.92)))
  (wire (pts (xy 201.93 121.92) (xy 201.93 123.19)))
  (wire (pts (xy 139.7 106.68) (xy 137.16 106.68)))
  (wire (pts (xy 139.7 111.76) (xy 137.16 111.76)))
  (wire (pts (xy 124.46 137.16) (xy 170.18 137.16)))
  (wire (pts (xy 173.99 121.92) (xy 173.99 137.16)))
  (wire (pts (xy 170.18 137.16) (xy 173.99 137.16)))
  (wire (pts (xy 177.8 129.54) (xy 177.8 137.16)))
  (wire (pts (xy 184.15 106.68) (xy 184.15 113.03)))
  (wire (pts (xy 173.99 137.16) (xy 177.8 137.16)))
  (wire (pts (xy 173.99 111.76) (xy 173.99 106.68)))
  (wire (pts (xy 184.15 120.65) (xy 184.15 137.16)))
  (wire (pts (xy 124.46 106.68) (xy 124.46 110.49)))
  (wire (pts (xy 170.18 106.68) (xy 173.99 106.68)))
  (hierarchical_label "VOUT" (shape input) (at 210.82 106.68 0) (fields_autoplaced))
  (hierarchical_label "GND" (shape input) (at 111.76 137.16 180) (fields_autoplaced))
  (hierarchical_label "VIN" (shape input) (at 110.49 106.68 180) (fields_autoplaced))
  (symbol (lib_id "Device:C") (at 177.8 125.73 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C11" (at 180.34 124.46 0))
    (property "Value" "1nF" (at 180.34 127 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 178.7652 129.54 0))
    (property "Datasheet" "~" (at 177.8 125.73 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C11") (unit 1)
        )
        (path
          (reference "C10") (unit 1)
        )
        (path
          (reference "C14") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "ADP7142ACPZN-R7:ADP7142ACPZN-R7") (at 154.94 114.3 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U10" (at 154.94 96.52 0))
    (property "Value" "ADP7142ACPZN3.3-R7" (at 154.94 99.06 0))
    (property "Footprint" "SON65P200X200X65-7N" (at 154.94 114.3 0))
    (property "Datasheet" "" (at 154.94 114.3 0))
    (property "PARTREV" "E" (at 154.94 114.3 0))
    (property "MF" "Analog Devices" (at 154.94 114.3 0))
    (property "SNAPEDA_PACKAGE_ID" "19057" (at 154.94 114.3 0))
    (property "STANDARD" "IPC-7351B" (at 154.94 114.3 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (instances
      (project "channelCard"
        (path
          (reference "U10") (unit 1)
        )
        (path
          (reference "U11") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 201.93 118.11 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R8" (at 204.47 116.84 0))
    (property "Value" "90" (at 204.47 119.38 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 200.152 118.11 90))
    (property "Datasheet" "~" (at 201.93 118.11 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R8") (unit 1)
        )
        (path
          (reference "R8") (unit 1)
        )
        (path
          (reference "R9") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED") (at 201.93 127 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "D3" (at 204.47 125.73 90))
    (property "Value" "LT Q39G-q100-25-1" (at 204.47 128.27 90))
    (property "Footprint" "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (at 201.93 127 0))
    (property "Datasheet" "~" (at 201.93 127 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "D3") (unit 1)
        )
        (path
          (reference "D3") (unit 1)
        )
        (path
          (reference "D5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 124.46 114.3 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C11" (at 127 113.03 0))
    (property "Value" "2.2uF" (at 127 115.57 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 125.4252 118.11 0))
    (property "Datasheet" "~" (at 124.46 114.3 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C11") (unit 1)
        )
        (path
          (reference "C27") (unit 1)
        )
        (path
          (reference "C28") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 184.15 116.84 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C11" (at 186.69 115.57 0))
    (property "Value" "2.2uF" (at 186.69 118.11 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 185.1152 120.65 0))
    (property "Datasheet" "~" (at 184.15 116.84 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C11") (unit 1)
        )
        (path
          (reference "C11") (unit 1)
        )
        (path
          (reference "C15") (unit 1)
        )
      )
    )
  )
)
