(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "2023-07-25_19-26-39:INA228AIDGSR" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 20.32 10.16 0))
      (property "Value" "INA228AIDGSR" (at 20.32 7.62 0))
      (property "Footprint" "VSSOP10_DGS_TEX" (at 0 0 0))
      (property "Datasheet" "INA228AIDGSR" (at 0 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "INA228AIDGSR" (at 0 0 0))
      (property "ki_fp_filters" "VSSOP10_DGS_TEX VSSOP10_DGS_TEX-M VSSOP10_DGS_TEX-L" (at 0 0 0))
      (symbol "INA228AIDGSR_0_1"
        (polyline
          (pts
            (xy 7.62 -15.24)
            (xy 33.02 -15.24)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 7.62 5.08)
            (xy 7.62 -15.24)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 33.02 -15.24)
            (xy 33.02 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 33.02 5.08)
            (xy 7.62 5.08)
          )
          (fill (type none))
        )
        (pin input line (at 0 0 0) (length 7.62)
          (name "A1")
          (number "1")
        )
        (pin input line (at 40.64 0 180) (length 7.62)
          (name "IN+")
          (number "10")
        )
        (pin input line (at 0 -2.54 0) (length 7.62)
          (name "A0")
          (number "2")
        )
        (pin output line (at 0 -5.08 0) (length 7.62)
          (name "ALERT")
          (number "3")
        )
        (pin bidirectional line (at 0 -7.62 0) (length 7.62)
          (name "SDA")
          (number "4")
        )
        (pin input line (at 0 -10.16 0) (length 7.62)
          (name "SCL")
          (number "5")
        )
        (pin power_in line (at 40.64 -10.16 180) (length 7.62)
          (name "VS")
          (number "6")
        )
        (pin power_out line (at 40.64 -7.62 180) (length 7.62)
          (name "GND")
          (number "7")
        )
        (pin power_in line (at 40.64 -5.08 180) (length 7.62)
          (name "VBUS")
          (number "8")
        )
        (pin input line (at 40.64 -2.54 180) (length 7.62)
          (name "IN-")
          (number "9")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.635 2.54 0))
      (property "Value" "C" (at 0.635 -2.54 0))
      (property "Footprint" "" (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (at 0 0 0))
      (property "ki_fp_filters" "C_*" (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "R" (at 0 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
  )
  (junction (at 92.71 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 143.51 85.09) (diameter 0) (color 0 0 0 0))
  (junction (at 152.4 85.09) (diameter 0) (color 0 0 0 0))
  (junction (at 151.13 92.71) (diameter 0) (color 0 0 0 0))
  (junction (at 92.71 72.39) (diameter 0) (color 0 0 0 0))
  (junction (at 116.84 72.39) (diameter 0) (color 0 0 0 0))
  (junction (at 143.51 72.39) (diameter 0) (color 0 0 0 0))
  (junction (at 116.84 85.09) (diameter 0) (color 0 0 0 0))
  (junction (at 99.06 72.39) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 151.13 92.71) (xy 151.13 95.25)))
  (wire (pts (xy 92.71 58.42) (xy 92.71 62.23)))
  (wire (pts (xy 153.67 85.09) (xy 152.4 85.09)))
  (wire (pts (xy 193.04 85.09) (xy 194.31 85.09)))
  (wire (pts (xy 131.064 85.09) (xy 116.84 85.09)))
  (wire (pts (xy 193.04 82.55) (xy 200.66 82.55)))
  (wire (pts (xy 92.71 90.17) (xy 152.4 90.17)))
  (wire (pts (xy 116.84 74.295) (xy 116.84 72.39)))
  (wire (pts (xy 92.71 109.22) (xy 92.71 90.17)))
  (wire (pts (xy 114.3 85.09) (xy 116.84 85.09)))
  (wire (pts (xy 92.71 72.39) (xy 92.71 74.93)))
  (wire (pts (xy 152.4 85.09) (xy 143.51 85.09)))
  (wire (pts (xy 99.06 87.63) (xy 152.4 87.63)))
  (wire (pts (xy 151.13 109.22) (xy 92.71 109.22)))
  (wire (pts (xy 198.12 90.17) (xy 193.04 90.17)))
  (wire (pts (xy 201.93 85.09) (xy 205.74 85.09)))
  (wire (pts (xy 116.84 81.915) (xy 116.84 85.09)))
  (wire (pts (xy 92.71 72.39) (xy 99.06 72.39)))
  (wire (pts (xy 152.4 92.71) (xy 151.13 92.71)))
  (wire (pts (xy 92.71 82.55) (xy 92.71 90.17)))
  (wire (pts (xy 99.06 87.63) (xy 99.06 72.39)))
  (wire (pts (xy 152.4 72.39) (xy 143.51 72.39)))
  (wire (pts (xy 152.4 82.55) (xy 152.4 72.39)))
  (wire (pts (xy 143.51 72.39) (xy 143.51 73.66)))
  (wire (pts (xy 92.71 90.17) (xy 88.9 90.17)))
  (wire (pts (xy 92.71 69.85) (xy 92.71 72.39)))
  (wire (pts (xy 131.064 72.39) (xy 116.84 72.39)))
  (wire (pts (xy 138.684 72.39) (xy 143.51 72.39)))
  (wire (pts (xy 151.13 109.22) (xy 151.13 102.87)))
  (wire (pts (xy 88.9 58.42) (xy 92.71 58.42)))
  (wire (pts (xy 138.684 85.09) (xy 143.51 85.09)))
  (wire (pts (xy 151.13 92.71) (xy 148.59 92.71)))
  (wire (pts (xy 198.12 92.71) (xy 193.04 92.71)))
  (wire (pts (xy 143.51 81.28) (xy 143.51 85.09)))
  (wire (pts (xy 99.06 72.39) (xy 116.84 72.39)))
  (label "GND" (at 200.66 82.55 0) (fields_autoplaced))
  (label "VS" (at 205.74 85.09 0) (fields_autoplaced))
  (hierarchical_label "SCL" (shape input) (at 198.12 92.71 0) (fields_autoplaced))
  (hierarchical_label "SDA" (shape input) (at 198.12 90.17 0) (fields_autoplaced))
  (hierarchical_label "Seawater" (shape input) (at 114.3 85.09 180) (fields_autoplaced))
  (hierarchical_label "Gnd" (shape input) (at 88.9 90.17 180) (fields_autoplaced))
  (hierarchical_label "Vin" (shape input) (at 88.9 58.42 180) (fields_autoplaced))
  (hierarchical_label "VS" (shape input) (at 148.59 92.71 180) (fields_autoplaced))
  (symbol (lib_id "Device:R") (at 92.71 66.04 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R11" (at 95.25 64.77 0))
    (property "Value" "4.7k" (at 95.25 67.31 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 94.488 66.04 90))
    (property "Datasheet" "~" (at 92.71 66.04 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R11") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 116.84 78.105 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R13" (at 119.38 76.835 0))
    (property "Value" "30 Ohm" (at 119.38 79.375 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 118.618 78.105 90))
    (property "Datasheet" "~" (at 116.84 78.105 0))
    (property "power" "0.1 Watt" (at 122.555 81.788 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R13") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 151.13 99.06 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C17" (at 147.32 97.79 0))
    (property "Value" "0.1uF" (at 147.32 100.33 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 150.1648 102.87 0))
    (property "Datasheet" "~" (at 151.13 99.06 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C17") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 198.12 85.09 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R16" (at 198.12 87.63 90))
    (property "Value" " 0 Ohm" (at 204.47 87.63 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 198.12 86.868 90))
    (property "Datasheet" "~" (at 198.12 85.09 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R16") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 143.51 77.47 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C18" (at 151.13 76.2 0))
    (property "Value" "0.1uF" (at 152.4 78.74 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 142.5448 81.28 0))
    (property "Datasheet" "~" (at 143.51 77.47 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C18") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 92.71 78.74 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R12" (at 90.17 77.47 0))
    (property "Value" "4.7k" (at 90.17 80.01 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 90.932 78.74 90))
    (property "Datasheet" "~" (at 92.71 78.74 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R12") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 134.874 72.39 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R14" (at 133.858 68.453 90))
    (property "Value" "10 Ohm" (at 135.763 70.358 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 134.874 74.168 90))
    (property "Datasheet" "~" (at 134.874 72.39 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R14") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 134.874 85.09 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R15" (at 133.477 80.264 90))
    (property "Value" "10 Ohm" (at 135.382 82.55 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 134.874 86.868 90))
    (property "Datasheet" "~" (at 134.874 85.09 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R15") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "2023-07-25_19-26-39:INA228AIDGSR") (at 193.04 82.55 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U3" (at 172.72 80.01 0))
    (property "Value" "INA228AIDGSR" (at 172.72 95.25 0))
    (property "Footprint" "VSSOP10_DGS_TEX" (at 193.04 82.55 0))
    (property "Datasheet" "INA228AIDGSR" (at 193.04 82.55 0))
    (pin "1")
    (pin "10")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "channelCard"
        (path
          (reference "U3") (unit 1)
        )
        (path
          (reference "U3") (unit 1)
        )
      )
    )
  )
)
