(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (title_block
    (title "Roadrunner")
    (date "2017-08-14")
    (rev "v1.1.2")
    (company "Jacob Miller")
    (comment 1 "Arduino compatible board based on TI's TM4C123G")
  )
  (lib_symbols
    (symbol "Roadrunner-rescue:+3.3V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+3.3V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (symbol "+3.3V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3.3V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3V3")
          (number "1")
        )
      )
    )
    (symbol "Roadrunner-rescue:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+5V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "Roadrunner-rescue:CONN_01X01" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 2.54 0))
      (property "Value" "CONN_01X01" (at 2.54 0 90))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_fp_filters" "Pin_Header_Straight_1X* Pin_Header_Angled_1X* Socket_Strip_Straight_1X* Socket_Strip_Angled_1X*" (at 0 0 0))
      (symbol "CONN_01X01_0_1"
        (rectangle (start -1.27 0.127) (end 0.254 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 1.27) (end 1.27 -1.27)
          (fill (type none))
        )
      )
      (symbol "CONN_01X01_1_1"
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "P1")
          (number "1")
        )
      )
    )
    (symbol "Roadrunner-rescue:CONN_01X02" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 3.81 0))
      (property "Value" "CONN_01X02" (at 2.54 0 90))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_fp_filters" "Pin_Header_Straight_1X* Pin_Header_Angled_1X* Socket_Strip_Straight_1X* Socket_Strip_Angled_1X*" (at 0 0 0))
      (symbol "CONN_01X02_0_1"
        (rectangle (start -1.27 -1.143) (end 0.254 -1.397)
          (fill (type none))
        )
        (rectangle (start -1.27 1.397) (end 0.254 1.143)
          (fill (type none))
        )
        (rectangle (start -1.27 2.54) (end 1.27 -2.54)
          (fill (type none))
        )
      )
      (symbol "CONN_01X02_1_1"
        (pin passive line (at -5.08 1.27 0) (length 3.81)
          (name "P1")
          (number "1")
        )
        (pin passive line (at -5.08 -1.27 0) (length 3.81)
          (name "P2")
          (number "2")
        )
      )
    )
    (symbol "Roadrunner-rescue:CONN_01X04" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 6.35 0))
      (property "Value" "CONN_01X04" (at 2.54 0 90))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_fp_filters" "Pin_Header_Straight_1X* Pin_Header_Angled_1X* Socket_Strip_Straight_1X* Socket_Strip_Angled_1X*" (at 0 0 0))
      (symbol "CONN_01X04_0_1"
        (rectangle (start -1.27 -3.683) (end 0.254 -3.937)
          (fill (type none))
        )
        (rectangle (start -1.27 -1.143) (end 0.254 -1.397)
          (fill (type none))
        )
        (rectangle (start -1.27 1.397) (end 0.254 1.143)
          (fill (type none))
        )
        (rectangle (start -1.27 3.937) (end 0.254 3.683)
          (fill (type none))
        )
        (rectangle (start -1.27 5.08) (end 1.27 -5.08)
          (fill (type none))
        )
      )
      (symbol "CONN_01X04_1_1"
        (pin passive line (at -5.08 3.81 0) (length 3.81)
          (name "P1")
          (number "1")
        )
        (pin passive line (at -5.08 1.27 0) (length 3.81)
          (name "P2")
          (number "2")
        )
        (pin passive line (at -5.08 -1.27 0) (length 3.81)
          (name "P3")
          (number "3")
        )
        (pin passive line (at -5.08 -3.81 0) (length 3.81)
          (name "P4")
          (number "4")
        )
      )
    )
    (symbol "Roadrunner-rescue:CONN_01X06" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 8.89 0))
      (property "Value" "CONN_01X06" (at 2.54 0 90))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_fp_filters" "Pin_Header_Straight_1X* Pin_Header_Angled_1X* Socket_Strip_Straight_1X* Socket_Strip_Angled_1X*" (at 0 0 0))
      (symbol "CONN_01X06_0_1"
        (rectangle (start -1.27 -6.223) (end 0.254 -6.477)
          (fill (type none))
        )
        (rectangle (start -1.27 -3.683) (end 0.254 -3.937)
          (fill (type none))
        )
        (rectangle (start -1.27 -1.143) (end 0.254 -1.397)
          (fill (type none))
        )
        (rectangle (start -1.27 1.397) (end 0.254 1.143)
          (fill (type none))
        )
        (rectangle (start -1.27 3.937) (end 0.254 3.683)
          (fill (type none))
        )
        (rectangle (start -1.27 6.477) (end 0.254 6.223)
          (fill (type none))
        )
        (rectangle (start -1.27 7.62) (end 1.27 -7.62)
          (fill (type none))
        )
      )
      (symbol "CONN_01X06_1_1"
        (pin passive line (at -5.08 6.35 0) (length 3.81)
          (name "P1")
          (number "1")
        )
        (pin passive line (at -5.08 3.81 0) (length 3.81)
          (name "P2")
          (number "2")
        )
        (pin passive line (at -5.08 1.27 0) (length 3.81)
          (name "P3")
          (number "3")
        )
        (pin passive line (at -5.08 -1.27 0) (length 3.81)
          (name "P4")
          (number "4")
        )
        (pin passive line (at -5.08 -3.81 0) (length 3.81)
          (name "P5")
          (number "5")
        )
        (pin passive line (at -5.08 -6.35 0) (length 3.81)
          (name "P6")
          (number "6")
        )
      )
    )
    (symbol "Roadrunner-rescue:CONN_01X08" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 11.43 0))
      (property "Value" "CONN_01X08" (at 2.54 0 90))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_fp_filters" "Pin_Header_Straight_1X* Pin_Header_Angled_1X* Socket_Strip_Straight_1X* Socket_Strip_Angled_1X*" (at 0 0 0))
      (symbol "CONN_01X08_0_1"
        (rectangle (start -1.27 -10.16) (end 1.27 10.16)
          (fill (type none))
        )
        (rectangle (start -1.27 -8.763) (end 0.254 -9.017)
          (fill (type none))
        )
        (rectangle (start -1.27 -6.223) (end 0.254 -6.477)
          (fill (type none))
        )
        (rectangle (start -1.27 -3.683) (end 0.254 -3.937)
          (fill (type none))
        )
        (rectangle (start -1.27 -1.143) (end 0.254 -1.397)
          (fill (type none))
        )
        (rectangle (start -1.27 1.397) (end 0.254 1.143)
          (fill (type none))
        )
        (rectangle (start -1.27 3.937) (end 0.254 3.683)
          (fill (type none))
        )
        (rectangle (start -1.27 6.477) (end 0.254 6.223)
          (fill (type none))
        )
        (rectangle (start -1.27 9.017) (end 0.254 8.763)
          (fill (type none))
        )
      )
      (symbol "CONN_01X08_1_1"
        (pin passive line (at -5.08 8.89 0) (length 3.81)
          (name "P1")
          (number "1")
        )
        (pin passive line (at -5.08 6.35 0) (length 3.81)
          (name "P2")
          (number "2")
        )
        (pin passive line (at -5.08 3.81 0) (length 3.81)
          (name "P3")
          (number "3")
        )
        (pin passive line (at -5.08 1.27 0) (length 3.81)
          (name "P4")
          (number "4")
        )
        (pin passive line (at -5.08 -1.27 0) (length 3.81)
          (name "P5")
          (number "5")
        )
        (pin passive line (at -5.08 -3.81 0) (length 3.81)
          (name "P6")
          (number "6")
        )
        (pin passive line (at -5.08 -6.35 0) (length 3.81)
          (name "P7")
          (number "7")
        )
        (pin passive line (at -5.08 -8.89 0) (length 3.81)
          (name "P8")
          (number "8")
        )
      )
    )
    (symbol "Roadrunner-rescue:CONN_01X10" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 13.97 0))
      (property "Value" "CONN_01X10" (at 2.54 0 90))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_fp_filters" "Pin_Header_Straight_1X* Pin_Header_Angled_1X* Socket_Strip_Straight_1X* Socket_Strip_Angled_1X*" (at 0 0 0))
      (symbol "CONN_01X10_0_1"
        (rectangle (start -1.27 -11.303) (end 0.254 -11.557)
          (fill (type none))
        )
        (rectangle (start -1.27 -8.763) (end 0.254 -9.017)
          (fill (type none))
        )
        (rectangle (start -1.27 -6.223) (end 0.254 -6.477)
          (fill (type none))
        )
        (rectangle (start -1.27 -3.683) (end 0.254 -3.937)
          (fill (type none))
        )
        (rectangle (start -1.27 -1.143) (end 0.254 -1.397)
          (fill (type none))
        )
        (rectangle (start -1.27 1.397) (end 0.254 1.143)
          (fill (type none))
        )
        (rectangle (start -1.27 3.937) (end 0.254 3.683)
          (fill (type none))
        )
        (rectangle (start -1.27 6.477) (end 0.254 6.223)
          (fill (type none))
        )
        (rectangle (start -1.27 9.017) (end 0.254 8.763)
          (fill (type none))
        )
        (rectangle (start -1.27 11.557) (end 0.254 11.303)
          (fill (type none))
        )
        (rectangle (start -1.27 12.7) (end 1.27 -12.7)
          (fill (type none))
        )
      )
      (symbol "CONN_01X10_1_1"
        (pin passive line (at -5.08 11.43 0) (length 3.81)
          (name "P1")
          (number "1")
        )
        (pin passive line (at -5.08 -11.43 0) (length 3.81)
          (name "P10")
          (number "10")
        )
        (pin passive line (at -5.08 8.89 0) (length 3.81)
          (name "P2")
          (number "2")
        )
        (pin passive line (at -5.08 6.35 0) (length 3.81)
          (name "P3")
          (number "3")
        )
        (pin passive line (at -5.08 3.81 0) (length 3.81)
          (name "P4")
          (number "4")
        )
        (pin passive line (at -5.08 1.27 0) (length 3.81)
          (name "P5")
          (number "5")
        )
        (pin passive line (at -5.08 -1.27 0) (length 3.81)
          (name "P6")
          (number "6")
        )
        (pin passive line (at -5.08 -3.81 0) (length 3.81)
          (name "P7")
          (number "7")
        )
        (pin passive line (at -5.08 -6.35 0) (length 3.81)
          (name "P8")
          (number "8")
        )
        (pin passive line (at -5.08 -8.89 0) (length 3.81)
          (name "P9")
          (number "9")
        )
      )
    )
    (symbol "Roadrunner-rescue:CP" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.635 2.54 0))
      (property "Value" "CP" (at 0.635 -2.54 0))
      (property "Footprint" "" (at 0.9652 -3.81 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_fp_filters" "CP_*" (at 0 0 0))
      (symbol "CP_0_1"
        (rectangle (start -2.286 0.508) (end -2.286 1.016)
          (fill (type none))
        )
        (rectangle (start -2.286 0.508) (end 2.286 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 2.286)
            (xy -0.762 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 2.794)
            (xy -1.27 1.778)
          )
          (fill (type none))
        )
        (rectangle (start 2.286 -0.508) (end -2.286 -1.016)
          (fill (type outline))
        )
        (rectangle (start 2.286 1.016) (end -2.286 1.016)
          (fill (type none))
        )
        (rectangle (start 2.286 1.016) (end 2.286 0.508)
          (fill (type none))
        )
      )
      (symbol "CP_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Roadrunner-rescue:C_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.254 1.778 0))
      (property "Value" "C_Small" (at 0.254 -2.032 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_fp_filters" "C_*" (at 0 0 0))
      (symbol "C_Small_0_1"
        (polyline
          (pts
            (xy -1.524 -0.508)
            (xy 1.524 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (fill (type none))
        )
      )
      (symbol "C_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Roadrunner-rescue:Crystal" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Y" (at 0 3.81 0))
      (property "Value" "Crystal" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_fp_filters" "Crystal*" (at 0 0 0))
      (symbol "Crystal_0_1"
        (rectangle (start -1.143 2.54) (end 1.143 -2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy -1.905 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.905 -1.27)
            (xy 1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 1.905 0)
          )
          (fill (type none))
        )
      )
      (symbol "Crystal_1_1"
        (pin passive line (at -3.81 0 0) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Roadrunner-rescue:GNDREF" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GNDREF" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (symbol "GNDREF_0_1"
        (polyline
          (pts
            (xy -0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.127 -2.54)
            (xy 0.127 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -1.27)
            (xy 0 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GNDREF_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GNDREF")
          (number "1")
        )
      )
    )
    (symbol "Roadrunner-rescue:HEADER_1" (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 3.81 0))
      (property "Value" "HEADER_1" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (symbol "HEADER_1_0_1"
        (rectangle (start 2.54 1.27) (end 0 -1.27)
          (fill (type none))
        )
      )
      (symbol "HEADER_1_1_1"
        (pin passive line (at -2.54 0 0) (length 2.54)
          (name "~")
          (number "1")
        )
      )
    )
    (symbol "Roadrunner-rescue:LED_ALT" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (at 0 2.54 0))
      (property "Value" "LED_ALT" (at 0 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_fp_filters" "LED*" (at 0 0 0))
      (symbol "LED_ALT_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_ALT_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Roadrunner-rescue:LM1117-3.3" (pin_names (offset 0.762)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 2.54 -6.35 0))
      (property "Value" "LM1117-3.3" (at 0 6.35 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_fp_filters" "SOT-223* TO-263* TO-252*" (at 0 0 0))
      (symbol "LM1117-3.3_0_1"
        (rectangle (start -5.08 -5.08) (end 5.08 5.08)
          (fill (type background))
        )
      )
      (symbol "LM1117-3.3_1_1"
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND/ADJ")
          (number "1")
        )
        (pin power_out line (at 7.62 0 180) (length 2.54)
          (name "VO")
          (number "2")
        )
        (pin power_in line (at -7.62 0 0) (length 2.54)
          (name "VI")
          (number "3")
        )
        (pin power_out line (at 7.62 0 180) (length 2.54) hide
          (name "VO")
          (number "4")
        )
      )
    )
    (symbol "Roadrunner-rescue:M_Hole" (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "T" (at 0 2.54 0))
      (property "Value" "M_Hole" (at 0 5.08 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (symbol "M_Hole_0_1"
        (circle (center 0 0) (radius 1.8034)
          (fill (type none))
        )
      )
    )
    (symbol "Roadrunner-rescue:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "R" (at 0 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_fp_filters" "R_* R_*" (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Roadrunner-rescue:R_Pack04" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "RN" (at -7.62 0 90))
      (property "Value" "R_Pack04" (at 5.08 0 90))
      (property "Footprint" "" (at 6.985 0 90))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_fp_filters" "DIP* SOIC*" (at 0 0 0))
      (symbol "R_Pack04_0_1"
        (rectangle (start -6.35 -2.413) (end 3.81 2.413)
          (fill (type background))
        )
        (rectangle (start -5.715 1.905) (end -4.445 -1.905)
          (fill (type none))
        )
        (rectangle (start -3.175 1.905) (end -1.905 -1.905)
          (fill (type none))
        )
        (rectangle (start -0.635 1.905) (end 0.635 -1.905)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 -2.54)
            (xy -5.08 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 1.905)
            (xy -5.08 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -2.54)
            (xy -2.54 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 1.905)
            (xy -2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -2.54)
            (xy 0 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.905)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 2.54 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.905)
            (xy 2.54 2.54)
          )
          (fill (type none))
        )
        (rectangle (start 1.905 1.905) (end 3.175 -1.905)
          (fill (type none))
        )
      )
      (symbol "R_Pack04_1_1"
        (pin passive line (at -5.08 -5.08 90) (length 2.54)
          (name "R1.1")
          (number "1")
        )
        (pin passive line (at -2.54 -5.08 90) (length 2.54)
          (name "R2.1")
          (number "2")
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "R3.1")
          (number "3")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "R4.1")
          (number "4")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "R4.2")
          (number "5")
        )
        (pin passive line (at 0 5.08 270) (length 2.54)
          (name "R3.2")
          (number "6")
        )
        (pin passive line (at -2.54 5.08 270) (length 2.54)
          (name "R2.2")
          (number "7")
        )
        (pin passive line (at -5.08 5.08 270) (length 2.54)
          (name "R1.2")
          (number "8")
        )
      )
    )
    (symbol "Roadrunner-rescue:SW_PUSH" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (at 0.254 3.048 0))
      (property "Value" "SW_PUSH" (at 0 -2.032 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (symbol "SW_PUSH_0_0"
        (rectangle (start -3.048 1.016) (end 3.048 1.27)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy -0.508 2.032)
            (xy 0.508 2.032)
            (xy 0.762 1.27)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "SW_PUSH_0_1"
        (pin passive inverted (at -3.81 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin passive inverted (at 3.81 0 180) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Roadrunner-rescue:TM4C123GH6PM" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -31.75 50.8 0))
      (property "Value" "TM4C123GH6PM" (at 16.51 50.8 0))
      (property "Footprint" "LQFP-64" (at 0 0 0))
      (property "Datasheet" "" (at 0 5.08 0))
      (property "ki_fp_filters" "LQFP-64*" (at 0 0 0))
      (symbol "TM4C123GH6PM_0_1"
        (rectangle (start -31.75 49.53) (end 31.75 -49.53)
          (fill (type background))
        )
      )
      (symbol "TM4C123GH6PM_1_1"
        (pin bidirectional line (at 35.56 7.62 180) (length 3.81)
          (name "SSI2RX/T0CCP0/PB6")
          (number "1")
        )
        (pin bidirectional line (at 35.56 -40.64 180) (length 3.81)
          (name "NMI/U2TX/WT5CCP1/PD7")
          (number "10")
        )
        (pin power_in line (at -2.54 53.34 270) (length 3.81)
          (name "VDD")
          (number "11")
        )
        (pin power_in line (at -5.08 -53.34 90) (length 3.81)
          (name "GND")
          (number "12")
        )
        (pin bidirectional line (at 35.56 -17.78 180) (length 3.81)
          (name "C0-/U3TX/WT1CCP1/PC7")
          (number "13")
        )
        (pin bidirectional line (at 35.56 -15.24 180) (length 3.81)
          (name "C0+/U3RX/WT1CCP0/PC6")
          (number "14")
        )
        (pin bidirectional line (at 35.56 -12.7 180) (length 3.81)
          (name "C1+/U1CTS/U1TX/U4TX/WT0CCP1/PC5")
          (number "15")
        )
        (pin bidirectional line (at 35.56 -10.16 180) (length 3.81)
          (name "C1-/U1RTS/U1RX/U4RX/WT0CCP0/PC4")
          (number "16")
        )
        (pin bidirectional line (at 35.56 45.72 180) (length 3.81)
          (name "U0RX/PA0")
          (number "17")
        )
        (pin bidirectional line (at 35.56 43.18 180) (length 3.81)
          (name "U0TX/PA1")
          (number "18")
        )
        (pin bidirectional line (at 35.56 40.64 180) (length 3.81)
          (name "SSI0CLK/PA2")
          (number "19")
        )
        (pin power_in line (at 10.16 53.34 270) (length 3.81)
          (name "VDDA")
          (number "2")
        )
        (pin bidirectional line (at 35.56 38.1 180) (length 3.81)
          (name "SSI0FSS/PA3")
          (number "20")
        )
        (pin bidirectional line (at 35.56 35.56 180) (length 3.81)
          (name "SSI0RX/PA4")
          (number "21")
        )
        (pin bidirectional line (at 35.56 33.02 180) (length 3.81)
          (name "SSI0TX/PA5")
          (number "22")
        )
        (pin bidirectional line (at 35.56 30.48 180) (length 3.81)
          (name "I2C1SCL/PA6")
          (number "23")
        )
        (pin bidirectional line (at 35.56 27.94 180) (length 3.81)
          (name "I2C1SDA/PA7")
          (number "24")
        )
        (pin power_in line (at -10.16 53.34 270) (length 3.81)
          (name "VDDC")
          (number "25")
        )
        (pin power_in line (at 0 53.34 270) (length 3.81)
          (name "VDD")
          (number "26")
        )
        (pin power_in line (at -2.54 -53.34 90) (length 3.81)
          (name "GND")
          (number "27")
        )
        (pin bidirectional line (at -35.56 27.94 0) (length 3.81)
          (name "PF0/T0CCP0/SSI1RX/U1RTS/CAN0RX/C0O/MNI")
          (number "28")
        )
        (pin bidirectional line (at -35.56 25.4 0) (length 3.81)
          (name "PF1/T0CCP1/SSI1TX/U1CTS/C1O/TRD1")
          (number "29")
        )
        (pin power_in line (at 7.62 -53.34 90) (length 3.81)
          (name "GNDA")
          (number "3")
        )
        (pin bidirectional line (at -35.56 22.86 0) (length 3.81)
          (name "PF2/T1CCP0/SSI1CLK/TRD0")
          (number "30")
        )
        (pin bidirectional line (at -35.56 20.32 0) (length 3.81)
          (name "PF3/T1CCP1/SSI1FSS/CAN0TX/TRCLK")
          (number "31")
        )
        (pin input line (at -35.56 -10.16 0) (length 3.81)
          (name "~{WAKE}")
          (number "32")
        )
        (pin open_collector line (at -35.56 -12.7 0) (length 3.81)
          (name "~{HIB}")
          (number "33")
        )
        (pin passive line (at -35.56 -20.32 0) (length 3.81)
          (name "XOSC0")
          (number "34")
        )
        (pin power_in line (at -10.16 -53.34 90) (length 3.81)
          (name "GNDX")
          (number "35")
        )
        (pin passive line (at -35.56 -25.4 0) (length 3.81)
          (name "XOSC1")
          (number "36")
        )
        (pin passive line (at -35.56 -33.02 0) (length 3.81)
          (name "VBAT")
          (number "37")
        )
        (pin input line (at -35.56 10.16 0) (length 3.81)
          (name "~{RST}")
          (number "38")
        )
        (pin bidirectional line (at 0 -53.34 90) (length 3.81)
          (name "GND")
          (number "39")
        )
        (pin bidirectional line (at 35.56 5.08 180) (length 3.81)
          (name "SSI2TX/T0CCP1/PB7")
          (number "4")
        )
        (pin passive line (at -35.56 2.54 0) (length 3.81)
          (name "OSC0")
          (number "40")
        )
        (pin passive line (at -35.56 -2.54 0) (length 3.81)
          (name "OSC1")
          (number "41")
        )
        (pin power_in line (at 2.54 53.34 270) (length 3.81)
          (name "VDD")
          (number "42")
        )
        (pin bidirectional line (at 35.56 -33.02 180) (length 3.81)
          (name "U6RX/WT4CCP0/PD4")
          (number "43")
        )
        (pin bidirectional line (at 35.56 -35.56 180) (length 3.81)
          (name "U6TX/WT4CCP1/PD5")
          (number "44")
        )
        (pin bidirectional line (at 35.56 22.86 180) (length 3.81)
          (name "U1RX/T2CCP0/PB0")
          (number "45")
        )
        (pin bidirectional line (at 35.56 20.32 180) (length 3.81)
          (name "U1TX/T2CCP1/PB1")
          (number "46")
        )
        (pin bidirectional line (at 35.56 17.78 180) (length 3.81)
          (name "I2C0SCL/T3CCP0/PB2")
          (number "47")
        )
        (pin bidirectional line (at 35.56 15.24 180) (length 3.81)
          (name "I2C0SDA/T3CCP1/PB3")
          (number "48")
        )
        (pin bidirectional line (at 35.56 -7.62 180) (length 3.81)
          (name "TDO/SWO/T5CCP1/PC3")
          (number "49")
        )
        (pin bidirectional line (at -35.56 17.78 0) (length 3.81)
          (name "PF4/T2CCP0")
          (number "5")
        )
        (pin bidirectional line (at 35.56 -5.08 180) (length 3.81)
          (name "TDI/T5CCP0/PC2")
          (number "50")
        )
        (pin bidirectional line (at 35.56 -2.54 180) (length 3.81)
          (name "TMS/SWDIO/T4CCP1/PC1")
          (number "51")
        )
        (pin bidirectional line (at 35.56 0 180) (length 3.81)
          (name "TCK/SWCLK/T4CCP0/PC0")
          (number "52")
        )
        (pin bidirectional line (at 35.56 -38.1 180) (length 3.81)
          (name "U2RX/WT5CCP0/PD6")
          (number "53")
        )
        (pin power_in line (at 5.08 53.34 270) (length 3.81)
          (name "VDD")
          (number "54")
        )
        (pin power_in line (at 2.54 -53.34 90) (length 3.81)
          (name "GND")
          (number "55")
        )
        (pin power_in line (at -7.62 53.34 270) (length 3.81)
          (name "VDDC")
          (number "56")
        )
        (pin bidirectional line (at 35.56 10.16 180) (length 3.81)
          (name "AIN11/CAN0TX/SSI2FSS/T1CCP1/PB5")
          (number "57")
        )
        (pin bidirectional line (at 35.56 12.7 180) (length 3.81)
          (name "AIN10/CAN0RX/SSI2CLK/T1CCP0/PB4")
          (number "58")
        )
        (pin bidirectional line (at -35.56 35.56 0) (length 3.81)
          (name "PE4/AIN9/U5RX/I2C2SCL/CAN0RX")
          (number "59")
        )
        (pin bidirectional line (at -35.56 38.1 0) (length 3.81)
          (name "PE3/AIN0")
          (number "6")
        )
        (pin bidirectional line (at -35.56 33.02 0) (length 3.81)
          (name "PE5/AIN8/U5TX/I2C2SDA/CAN0TX")
          (number "60")
        )
        (pin bidirectional line (at 35.56 -22.86 180) (length 3.81)
          (name "AIN7/I2C3SCL/SSI1CLK/SSI3CLK/WT2CCP0/PD0")
          (number "61")
        )
        (pin bidirectional line (at 35.56 -25.4 180) (length 3.81)
          (name "AIN6/I2C3SDA/SSI1FSS/SSI3FSS/WT2CCP1/PD1")
          (number "62")
        )
        (pin bidirectional line (at 35.56 -27.94 180) (length 3.81)
          (name "AIN5/SSI1RX/SSI3RX/WT3CCP0/PD2")
          (number "63")
        )
        (pin bidirectional line (at 35.56 -30.48 180) (length 3.81)
          (name "AIN4/SSI1TX/SSI3TX/WT3CCP1/PD3")
          (number "64")
        )
        (pin bidirectional line (at -35.56 40.64 0) (length 3.81)
          (name "PE2/AIN1")
          (number "7")
        )
        (pin bidirectional line (at -35.56 43.18 0) (length 3.81)
          (name "PE1/AIN2/U7TX")
          (number "8")
        )
        (pin bidirectional line (at -35.56 45.72 0) (length 3.81)
          (name "PE0/AIN3/U7RX")
          (number "9")
        )
      )
    )
    (symbol "Roadrunner-rescue:UM6K33N" (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (at -5.08 10.795 0))
      (property "Value" "UM6K33N" (at -5.08 8.89 0))
      (property "Footprint" "Packages_SMD:SOT-363" (at -5.08 6.985 0))
      (property "Datasheet" "" (at 5.08 15.24 0))
      (property "ki_fp_filters" "SOT-36* SC-88 UMT6" (at 0 0 0))
      (symbol "UM6K33N_0_1"
        (rectangle (start -7.62 6.35) (end 7.62 -6.35)
          (fill (type background))
        )
        (circle (center -3.81 1.27) (radius 2.8194)
          (fill (type none))
        )
        (circle (center -2.54 0) (radius 0.127)
          (fill (type none))
        )
        (circle (center -2.54 2.54) (radius 0.127)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -7.62 0)
            (xy -5.08 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.445 0.254)
            (xy -4.445 -0.381)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.445 1.651)
            (xy -4.445 0.889)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.445 2.921)
            (xy -4.445 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -2.54)
            (xy -2.54 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 5.08)
            (xy -7.62 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 5.08)
            (xy -2.54 3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 1.651)
            (xy -2.159 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 1.651)
            (xy -1.524 1.651)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 1.651)
            (xy -1.397 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 1.651)
            (xy 1.397 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.032 1.651)
            (xy 1.524 1.651)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.032 1.651)
            (xy 2.159 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 2.54 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 5.08)
            (xy 2.54 3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 5.08)
            (xy 7.62 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.445 0.254)
            (xy 4.445 -0.381)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.445 1.651)
            (xy 4.445 0.889)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.445 2.921)
            (xy 4.445 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 7.62 0)
            (xy 5.08 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 2.794)
            (xy -5.08 -0.254)
            (xy -5.08 -0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -2.54)
            (xy -2.54 -5.08)
            (xy -7.62 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 2.54 -5.08)
            (xy 7.62 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 2.794)
            (xy 5.08 -0.254)
            (xy 5.08 -0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.318 0)
            (xy -2.54 0)
            (xy -2.54 -1.27)
            (xy -2.54 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.318 2.54)
            (xy -2.54 2.54)
            (xy -2.54 3.81)
            (xy -2.54 3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 2.54)
            (xy -1.778 2.54)
            (xy -1.778 0)
            (xy -2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 1.651)
            (xy -2.032 1.016)
            (xy -1.524 1.016)
            (xy -1.778 1.651)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 1.778 1.651)
            (xy 2.032 1.016)
            (xy 1.524 1.016)
            (xy 1.778 1.651)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy 1.778 2.54)
            (xy 1.778 0)
            (xy 2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.318 0)
            (xy 2.54 0)
            (xy 2.54 -1.27)
            (xy 2.54 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.318 2.54)
            (xy 2.54 2.54)
            (xy 2.54 3.81)
            (xy 2.54 3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.191 1.27)
            (xy -3.175 1.651)
            (xy -3.175 0.889)
            (xy -4.191 1.27)
            (xy -4.064 1.27)
            (xy -4.064 1.27)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 4.191 1.27)
            (xy 3.175 1.651)
            (xy 3.175 0.889)
            (xy 4.191 1.27)
            (xy 4.064 1.27)
            (xy 4.064 1.27)
          )
          (fill (type outline))
        )
        (circle (center 2.54 0) (radius 0.127)
          (fill (type none))
        )
        (circle (center 2.54 2.54) (radius 0.127)
          (fill (type none))
        )
        (circle (center 3.81 1.27) (radius 2.8194)
          (fill (type none))
        )
      )
      (symbol "UM6K33N_1_1"
        (polyline
          (pts
            (xy -4.318 1.27)
            (xy -3.81 1.27)
            (xy -2.54 1.27)
            (xy -2.54 0)
            (xy -2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.318 1.27)
            (xy 3.81 1.27)
            (xy 2.54 1.27)
            (xy 2.54 0)
            (xy 2.54 0)
          )
          (fill (type none))
        )
        (pin passive line (at -10.16 -5.08 0) (length 2.54)
          (name "S1")
          (number "1")
        )
        (pin passive line (at -10.16 0 0) (length 2.54)
          (name "G1")
          (number "2")
        )
        (pin passive line (at 10.16 5.08 180) (length 2.54)
          (name "D2")
          (number "3")
        )
        (pin passive line (at 10.16 -5.08 180) (length 2.54)
          (name "S2")
          (number "4")
        )
        (pin passive line (at 10.16 0 180) (length 2.54)
          (name "G2")
          (number "5")
        )
        (pin passive line (at -10.16 5.08 0) (length 2.54)
          (name "D1")
          (number "6")
        )
      )
    )
    (symbol "Roadrunner-rescue:USB_OTG" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at -5.08 11.43 0))
      (property "Value" "USB_OTG" (at -5.08 8.89 0))
      (property "Footprint" "" (at 3.81 -1.27 0))
      (property "Datasheet" "" (at 3.81 -1.27 0))
      (property "ki_fp_filters" "USB*" (at 0 0 0))
      (symbol "USB_OTG_0_1"
        (rectangle (start -5.08 -7.62) (end 5.08 7.62)
          (fill (type background))
        )
        (circle (center -3.81 2.159) (radius 0.635)
          (fill (type outline))
        )
        (circle (center -0.635 3.429) (radius 0.381)
          (fill (type outline))
        )
        (rectangle (start -0.127 -7.62) (end 0.127 -6.858)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 2.159)
            (xy 0.635 2.159)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.175 2.159)
            (xy -2.54 2.159)
            (xy -1.27 3.429)
            (xy -0.635 3.429)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 2.159)
            (xy -1.905 2.159)
            (xy -1.27 0.889)
            (xy 0 0.889)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 2.794)
            (xy 0.635 1.524)
            (xy 1.905 2.159)
            (xy 0.635 2.794)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -4.318 5.588)
            (xy -1.778 5.588)
            (xy -2.032 4.826)
            (xy -4.064 4.826)
            (xy -4.318 5.588)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -4.699 5.842)
            (xy -4.699 5.588)
            (xy -4.445 4.826)
            (xy -4.445 4.572)
            (xy -1.651 4.572)
            (xy -1.651 4.826)
            (xy -1.397 5.588)
            (xy -1.397 5.842)
            (xy -4.699 5.842)
          )
          (fill (type none))
        )
        (rectangle (start 0.254 1.27) (end -0.508 0.508)
          (fill (type outline))
        )
        (rectangle (start 5.08 -5.207) (end 4.318 -4.953)
          (fill (type none))
        )
        (rectangle (start 5.08 -2.667) (end 4.318 -2.413)
          (fill (type none))
        )
        (rectangle (start 5.08 -0.127) (end 4.318 0.127)
          (fill (type none))
        )
        (rectangle (start 5.08 4.953) (end 4.318 5.207)
          (fill (type none))
        )
      )
      (symbol "USB_OTG_1_1"
        (pin power_in line (at 7.62 5.08 180) (length 2.54)
          (name "VBUS")
          (number "1")
        )
        (pin passive line (at 7.62 -2.54 180) (length 2.54)
          (name "D-")
          (number "2")
        )
        (pin passive line (at 7.62 0 180) (length 2.54)
          (name "D+")
          (number "3")
        )
        (pin passive line (at 7.62 -5.08 180) (length 2.54)
          (name "ID")
          (number "4")
        )
        (pin power_in line (at 0 -10.16 90) (length 2.54)
          (name "GND")
          (number "5")
        )
        (pin passive line (at -2.54 -10.16 90) (length 2.54)
          (name "Shield")
          (number "6")
        )
      )
    )
  )
  (junction (at 119.38 191.77) (diameter 0) (color 0 0 0 0))
  (junction (at 135.89 140.97) (diameter 0) (color 0 0 0 0))
  (junction (at 252.73 49.53) (diameter 0) (color 0 0 0 0))
  (junction (at 73.66 113.03) (diameter 0) (color 0 0 0 0))
  (junction (at 149.86 191.77) (diameter 0) (color 0 0 0 0))
  (junction (at 134.62 191.77) (diameter 0) (color 0 0 0 0))
  (junction (at 127 191.77) (diameter 0) (color 0 0 0 0))
  (junction (at 111.76 20.32) (diameter 0) (color 0 0 0 0))
  (junction (at 157.48 184.15) (diameter 0) (color 0 0 0 0))
  (junction (at 125.73 172.72) (diameter 0) (color 0 0 0 0))
  (junction (at 205.74 149.86) (diameter 0) (color 0 0 0 0))
  (junction (at 127 184.15) (diameter 0) (color 0 0 0 0))
  (junction (at 20.32 124.46) (diameter 0) (color 0 0 0 0))
  (junction (at 91.44 113.03) (diameter 0) (color 0 0 0 0))
  (junction (at 143.51 22.86) (diameter 0) (color 0 0 0 0))
  (junction (at 46.99 31.75) (diameter 0) (color 0 0 0 0))
  (junction (at 39.37 167.64) (diameter 0) (color 0 0 0 0))
  (junction (at 142.24 191.77) (diameter 0) (color 0 0 0 0))
  (junction (at 114.3 161.29) (diameter 0) (color 0 0 0 0))
  (junction (at 149.86 184.15) (diameter 0) (color 0 0 0 0))
  (junction (at 157.48 191.77) (diameter 0) (color 0 0 0 0))
  (junction (at 226.06 152.4) (diameter 0) (color 0 0 0 0))
  (junction (at 205.74 152.4) (diameter 0) (color 0 0 0 0))
  (junction (at 138.43 26.67) (diameter 0) (color 0 0 0 0))
  (junction (at 226.06 149.86) (diameter 0) (color 0 0 0 0))
  (junction (at 140.97 143.51) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 20.32) (diameter 0) (color 0 0 0 0))
  (junction (at 119.38 20.32) (diameter 0) (color 0 0 0 0))
  (junction (at 205.74 147.32) (diameter 0) (color 0 0 0 0))
  (junction (at 76.2 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 88.9 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 226.06 154.94) (diameter 0) (color 0 0 0 0))
  (junction (at 38.1 31.75) (diameter 0) (color 0 0 0 0))
  (junction (at 143.51 26.67) (diameter 0) (color 0 0 0 0))
  (junction (at 135.89 161.29) (diameter 0) (color 0 0 0 0))
  (junction (at 119.38 27.94) (diameter 0) (color 0 0 0 0))
  (junction (at 142.24 184.15) (diameter 0) (color 0 0 0 0))
  (junction (at 138.43 140.97) (diameter 0) (color 0 0 0 0))
  (junction (at 252.73 46.99) (diameter 0) (color 0 0 0 0))
  (junction (at 252.73 44.45) (diameter 0) (color 0 0 0 0))
  (junction (at 39.37 50.8) (diameter 0) (color 0 0 0 0))
  (junction (at 82.55 113.03) (diameter 0) (color 0 0 0 0))
  (junction (at 134.62 184.15) (diameter 0) (color 0 0 0 0))
  (junction (at 119.38 184.15) (diameter 0) (color 0 0 0 0))
  (junction (at 111.76 27.94) (diameter 0) (color 0 0 0 0))
  (junction (at 140.97 140.97) (diameter 0) (color 0 0 0 0))
  (junction (at 140.97 26.67) (diameter 0) (color 0 0 0 0))
  (no_connect (at 40.64 154.94))
  (wire (pts (xy 27.94 118.11) (xy 41.91 118.11)))
  (wire (pts (xy 76.2 86.36) (xy 76.2 87.63)))
  (wire (pts (xy 102.87 55.88) (xy 101.6 55.88)))
  (wire (pts (xy 63.5 180.34) (xy 73.66 180.34)))
  (polyline (pts (xy 207.01 67.31) (xy 233.68 67.31)))
  (wire (pts (xy 102.87 60.96) (xy 101.6 60.96)))
  (wire (pts (xy 135.89 26.67) (xy 135.89 30.48)))
  (wire (pts (xy 274.32 104.14) (xy 270.51 104.14)))
  (wire (pts (xy 173.99 99.06) (xy 196.85 99.06)))
  (wire (pts (xy 101.6 63.5) (xy 102.87 63.5)))
  (wire (pts (xy 40.64 187.96) (xy 29.21 187.96)))
  (wire (pts (xy 29.21 190.5) (xy 40.64 190.5)))
  (wire (pts (xy 127 184.15) (xy 134.62 184.15)))
  (wire (pts (xy 29.21 185.42) (xy 40.64 185.42)))
  (wire (pts (xy 180.34 55.88) (xy 173.99 55.88)))
  (polyline (pts (xy 283.21 13.97) (xy 283.21 26.67)))
  (wire (pts (xy 111.76 20.32) (xy 119.38 20.32)))
  (wire (pts (xy 41.91 83.82) (xy 34.29 83.82)))
  (wire (pts (xy 140.97 30.48) (xy 140.97 26.67)))
  (wire (pts (xy 173.99 78.74) (xy 198.12 78.74)))
  (wire (pts (xy 157.48 185.42) (xy 157.48 184.15)))
  (wire (pts (xy 138.43 140.97) (xy 140.97 140.97)))
  (wire (pts (xy 104.14 27.94) (xy 111.76 27.94)))
  (wire (pts (xy 157.48 184.15) (xy 165.1 184.15)))
  (wire (pts (xy 226.06 147.32) (xy 228.6 147.32)))
  (wire (pts (xy 102.87 73.66) (xy 101.6 73.66)))
  (wire (pts (xy 228.6 149.86) (xy 226.06 149.86)))
  (wire (pts (xy 73.66 113.03) (xy 74.93 113.03)))
  (wire (pts (xy 73.66 113.03) (xy 73.66 119.38)))
  (wire (pts (xy 173.99 63.5) (xy 198.12 63.5)))
  (wire (pts (xy 76.2 81.28) (xy 76.2 86.36)))
  (wire (pts (xy 34.29 50.8) (xy 39.37 50.8)))
  (wire (pts (xy 271.78 109.22) (xy 270.51 109.22)))
  (wire (pts (xy 20.32 124.46) (xy 20.32 125.73)))
  (polyline (pts (xy 242.57 13.97) (xy 242.57 26.67)))
  (wire (pts (xy 173.99 38.1) (xy 180.34 38.1)))
  (wire (pts (xy 252.73 43.18) (xy 252.73 44.45)))
  (wire (pts (xy 34.29 162.56) (xy 34.29 149.86)))
  (wire (pts (xy 149.86 182.88) (xy 149.86 184.15)))
  (wire (pts (xy 274.32 71.12) (xy 274.32 68.58)))
  (wire (pts (xy 274.32 71.12) (xy 270.51 71.12)))
  (polyline (pts (xy 233.68 67.31) (xy 233.68 57.15)))
  (wire (pts (xy 246.38 88.9) (xy 246.38 91.44)))
  (wire (pts (xy 49.53 118.11) (xy 50.8 118.11)))
  (wire (pts (xy 63.5 160.02) (xy 76.2 160.02)))
  (wire (pts (xy 119.38 184.15) (xy 127 184.15)))
  (wire (pts (xy 208.28 152.4) (xy 205.74 152.4)))
  (wire (pts (xy 85.09 152.4) (xy 85.09 153.67)))
  (wire (pts (xy 39.37 49.53) (xy 39.37 50.8)))
  (wire (pts (xy 76.2 92.71) (xy 76.2 93.98)))
  (wire (pts (xy 173.99 109.22) (xy 180.34 109.22)))
  (wire (pts (xy 248.92 81.28) (xy 250.19 81.28)))
  (wire (pts (xy 34.29 74.93) (xy 38.1 74.93)))
  (wire (pts (xy 102.87 40.64) (xy 101.6 40.64)))
  (wire (pts (xy 40.64 157.48) (xy 39.37 157.48)))
  (wire (pts (xy 173.99 91.44) (xy 204.47 91.44)))
  (wire (pts (xy 63.5 152.4) (xy 85.09 152.4)))
  (wire (pts (xy 128.27 20.32) (xy 128.27 30.48)))
  (wire (pts (xy 17.78 123.19) (xy 17.78 124.46)))
  (wire (pts (xy 102.87 38.1) (xy 101.6 38.1)))
  (wire (pts (xy 127 184.15) (xy 127 185.42)))
  (wire (pts (xy 165.1 184.15) (xy 165.1 185.42)))
  (wire (pts (xy 146.05 140.97) (xy 146.05 137.16)))
  (wire (pts (xy 135.89 140.97) (xy 138.43 140.97)))
  (wire (pts (xy 173.99 106.68) (xy 180.34 106.68)))
  (wire (pts (xy 142.24 191.77) (xy 149.86 191.77)))
  (wire (pts (xy 205.74 154.94) (xy 208.28 154.94)))
  (polyline (pts (xy 242.57 20.32) (xy 283.21 20.32)))
  (wire (pts (xy 125.73 172.72) (xy 125.73 173.99)))
  (wire (pts (xy 125.73 172.72) (xy 135.89 172.72)))
  (wire (pts (xy 119.38 26.67) (xy 119.38 27.94)))
  (wire (pts (xy 173.99 53.34) (xy 180.34 53.34)))
  (wire (pts (xy 274.32 88.9) (xy 274.32 91.44)))
  (wire (pts (xy 140.97 137.16) (xy 140.97 140.97)))
  (wire (pts (xy 119.38 191.77) (xy 119.38 190.5)))
  (wire (pts (xy 80.01 86.36) (xy 76.2 86.36)))
  (wire (pts (xy 40.64 177.8) (xy 29.21 177.8)))
  (wire (pts (xy 80.01 113.03) (xy 82.55 113.03)))
  (wire (pts (xy 165.1 191.77) (xy 165.1 190.5)))
  (wire (pts (xy 173.99 83.82) (xy 204.47 83.82)))
  (wire (pts (xy 102.87 48.26) (xy 101.6 48.26)))
  (wire (pts (xy 135.89 157.48) (xy 135.89 161.29)))
  (wire (pts (xy 140.97 140.97) (xy 140.97 143.51)))
  (wire (pts (xy 36.83 167.64) (xy 39.37 167.64)))
  (wire (pts (xy 133.35 161.29) (xy 135.89 161.29)))
  (wire (pts (xy 146.05 143.51) (xy 140.97 143.51)))
  (wire (pts (xy 173.99 48.26) (xy 198.12 48.26)))
  (wire (pts (xy 173.99 116.84) (xy 180.34 116.84)))
  (wire (pts (xy 102.87 81.28) (xy 76.2 81.28)))
  (wire (pts (xy 173.99 124.46) (xy 196.85 124.46)))
  (wire (pts (xy 138.43 137.16) (xy 138.43 140.97)))
  (wire (pts (xy 205.74 149.86) (xy 205.74 152.4)))
  (polyline (pts (xy 283.21 26.67) (xy 242.57 26.67)))
  (wire (pts (xy 114.3 161.29) (xy 118.11 161.29)))
  (wire (pts (xy 63.5 144.78) (xy 73.66 144.78)))
  (wire (pts (xy 101.6 50.8) (xy 102.87 50.8)))
  (wire (pts (xy 142.24 184.15) (xy 149.86 184.15)))
  (wire (pts (xy 228.6 152.4) (xy 226.06 152.4)))
  (wire (pts (xy 17.78 124.46) (xy 20.32 124.46)))
  (wire (pts (xy 63.5 167.64) (xy 73.66 167.64)))
  (wire (pts (xy 138.43 30.48) (xy 138.43 26.67)))
  (wire (pts (xy 119.38 191.77) (xy 127 191.77)))
  (wire (pts (xy 173.99 114.3) (xy 180.34 114.3)))
  (wire (pts (xy 226.06 152.4) (xy 226.06 149.86)))
  (wire (pts (xy 102.87 45.72) (xy 101.6 45.72)))
  (wire (pts (xy 63.5 175.26) (xy 73.66 175.26)))
  (wire (pts (xy 135.89 137.16) (xy 135.89 140.97)))
  (wire (pts (xy 138.43 26.67) (xy 140.97 26.67)))
  (wire (pts (xy 87.63 86.36) (xy 88.9 86.36)))
  (wire (pts (xy 63.5 149.86) (xy 73.66 149.86)))
  (wire (pts (xy 119.38 27.94) (xy 119.38 29.21)))
  (wire (pts (xy 246.38 99.06) (xy 250.19 99.06)))
  (wire (pts (xy 34.29 31.75) (xy 38.1 31.75)))
  (wire (pts (xy 88.9 93.98) (xy 88.9 92.71)))
  (wire (pts (xy 111.76 184.15) (xy 119.38 184.15)))
  (wire (pts (xy 173.99 76.2) (xy 198.12 76.2)))
  (wire (pts (xy 38.1 22.86) (xy 38.1 20.32)))
  (wire (pts (xy 127 191.77) (xy 134.62 191.77)))
  (wire (pts (xy 40.64 182.88) (xy 29.21 182.88)))
  (wire (pts (xy 252.73 44.45) (xy 252.73 46.99)))
  (wire (pts (xy 27.94 113.03) (xy 29.21 113.03)))
  (wire (pts (xy 96.52 66.04) (xy 102.87 66.04)))
  (wire (pts (xy 248.92 109.22) (xy 250.19 109.22)))
  (wire (pts (xy 46.99 29.21) (xy 46.99 31.75)))
  (wire (pts (xy 63.5 190.5) (xy 73.66 190.5)))
  (wire (pts (xy 63.5 182.88) (xy 73.66 182.88)))
  (wire (pts (xy 133.35 137.16) (xy 133.35 140.97)))
  (wire (pts (xy 173.99 96.52) (xy 196.85 96.52)))
  (wire (pts (xy 173.99 121.92) (xy 196.85 121.92)))
  (wire (pts (xy 246.38 68.58) (xy 246.38 71.12)))
  (wire (pts (xy 149.86 191.77) (xy 149.86 193.04)))
  (wire (pts (xy 104.14 20.32) (xy 104.14 21.59)))
  (wire (pts (xy 180.34 68.58) (xy 173.99 68.58)))
  (wire (pts (xy 127 191.77) (xy 127 190.5)))
  (wire (pts (xy 119.38 184.15) (xy 119.38 185.42)))
  (wire (pts (xy 50.8 50.8) (xy 48.26 50.8)))
  (wire (pts (xy 40.64 162.56) (xy 34.29 162.56)))
  (wire (pts (xy 34.29 63.5) (xy 38.1 63.5)))
  (wire (pts (xy 173.99 60.96) (xy 198.12 60.96)))
  (wire (pts (xy 246.38 104.14) (xy 250.19 104.14)))
  (wire (pts (xy 134.62 184.15) (xy 142.24 184.15)))
  (wire (pts (xy 63.5 154.94) (xy 76.2 154.94)))
  (wire (pts (xy 173.99 43.18) (xy 198.12 43.18)))
  (wire (pts (xy 20.32 123.19) (xy 20.32 124.46)))
  (wire (pts (xy 274.32 99.06) (xy 270.51 99.06)))
  (wire (pts (xy 149.86 184.15) (xy 149.86 185.42)))
  (polyline (pts (xy 233.68 57.15) (xy 207.01 57.15)))
  (wire (pts (xy 246.38 58.42) (xy 246.38 60.96)))
  (wire (pts (xy 63.5 157.48) (xy 76.2 157.48)))
  (wire (pts (xy 246.38 76.2) (xy 250.19 76.2)))
  (wire (pts (xy 88.9 86.36) (xy 102.87 86.36)))
  (wire (pts (xy 142.24 184.15) (xy 142.24 185.42)))
  (wire (pts (xy 148.59 22.86) (xy 143.51 22.86)))
  (wire (pts (xy 135.89 26.67) (xy 138.43 26.67)))
  (wire (pts (xy 102.87 43.18) (xy 101.6 43.18)))
  (wire (pts (xy 63.5 177.8) (xy 73.66 177.8)))
  (wire (pts (xy 27.94 115.57) (xy 29.21 115.57)))
  (wire (pts (xy 114.3 172.72) (xy 125.73 172.72)))
  (wire (pts (xy 208.28 149.86) (xy 205.74 149.86)))
  (wire (pts (xy 173.99 50.8) (xy 198.12 50.8)))
  (wire (pts (xy 180.34 71.12) (xy 173.99 71.12)))
  (wire (pts (xy 91.44 113.03) (xy 91.44 119.38)))
  (wire (pts (xy 274.32 76.2) (xy 270.51 76.2)))
  (wire (pts (xy 134.62 184.15) (xy 134.62 185.42)))
  (wire (pts (xy 252.73 46.99) (xy 255.27 46.99)))
  (wire (pts (xy 63.5 147.32) (xy 73.66 147.32)))
  (wire (pts (xy 133.35 140.97) (xy 135.89 140.97)))
  (wire (pts (xy 149.86 191.77) (xy 157.48 191.77)))
  (wire (pts (xy 252.73 44.45) (xy 255.27 44.45)))
  (wire (pts (xy 102.87 96.52) (xy 101.6 96.52)))
  (wire (pts (xy 104.14 26.67) (xy 104.14 27.94)))
  (wire (pts (xy 111.76 184.15) (xy 111.76 185.42)))
  (wire (pts (xy 119.38 20.32) (xy 128.27 20.32)))
  (wire (pts (xy 111.76 20.32) (xy 111.76 21.59)))
  (wire (pts (xy 246.38 71.12) (xy 250.19 71.12)))
  (polyline (pts (xy 283.21 13.97) (xy 242.57 13.97)))
  (wire (pts (xy 125.73 168.91) (xy 125.73 172.72)))
  (wire (pts (xy 38.1 31.75) (xy 46.99 31.75)))
  (wire (pts (xy 63.5 185.42) (xy 73.66 185.42)))
  (wire (pts (xy 40.64 160.02) (xy 21.59 160.02)))
  (wire (pts (xy 173.99 88.9) (xy 204.47 88.9)))
  (wire (pts (xy 134.62 191.77) (xy 142.24 191.77)))
  (wire (pts (xy 111.76 191.77) (xy 111.76 190.5)))
  (wire (pts (xy 135.89 161.29) (xy 138.43 161.29)))
  (wire (pts (xy 157.48 190.5) (xy 157.48 191.77)))
  (wire (pts (xy 135.89 161.29) (xy 135.89 163.83)))
  (wire (pts (xy 102.87 93.98) (xy 101.6 93.98)))
  (wire (pts (xy 91.44 109.22) (xy 102.87 109.22)))
  (wire (pts (xy 142.24 191.77) (xy 142.24 190.5)))
  (wire (pts (xy 252.73 52.07) (xy 255.27 52.07)))
  (wire (pts (xy 39.37 170.18) (xy 39.37 167.64)))
  (wire (pts (xy 173.99 101.6) (xy 196.85 101.6)))
  (wire (pts (xy 143.51 26.67) (xy 143.51 30.48)))
  (wire (pts (xy 102.87 104.14) (xy 73.66 104.14)))
  (wire (pts (xy 73.66 104.14) (xy 73.66 113.03)))
  (wire (pts (xy 111.76 26.67) (xy 111.76 27.94)))
  (wire (pts (xy 114.3 161.29) (xy 114.3 163.83)))
  (wire (pts (xy 46.99 31.75) (xy 50.8 31.75)))
  (wire (pts (xy 63.5 165.1) (xy 73.66 165.1)))
  (wire (pts (xy 173.99 45.72) (xy 198.12 45.72)))
  (wire (pts (xy 40.64 170.18) (xy 39.37 170.18)))
  (wire (pts (xy 91.44 109.22) (xy 91.44 113.03)))
  (wire (pts (xy 128.27 140.97) (xy 128.27 137.16)))
  (wire (pts (xy 63.5 162.56) (xy 76.2 162.56)))
  (wire (pts (xy 88.9 86.36) (xy 88.9 87.63)))
  (wire (pts (xy 25.4 31.75) (xy 25.4 33.02)))
  (wire (pts (xy 39.37 167.64) (xy 40.64 167.64)))
  (wire (pts (xy 130.81 20.32) (xy 130.81 30.48)))
  (wire (pts (xy 205.74 147.32) (xy 205.74 149.86)))
  (wire (pts (xy 40.64 172.72) (xy 29.21 172.72)))
  (wire (pts (xy 50.8 48.26) (xy 50.8 50.8)))
  (polyline (pts (xy 207.01 57.15) (xy 207.01 67.31)))
  (wire (pts (xy 271.78 81.28) (xy 270.51 81.28)))
  (wire (pts (xy 205.74 152.4) (xy 205.74 154.94)))
  (wire (pts (xy 39.37 157.48) (xy 39.37 149.86)))
  (wire (pts (xy 140.97 143.51) (xy 140.97 144.78)))
  (wire (pts (xy 38.1 31.75) (xy 38.1 30.48)))
  (wire (pts (xy 134.62 191.77) (xy 134.62 190.5)))
  (wire (pts (xy 173.99 93.98) (xy 196.85 93.98)))
  (wire (pts (xy 111.76 161.29) (xy 114.3 161.29)))
  (wire (pts (xy 226.06 157.48) (xy 226.06 154.94)))
  (wire (pts (xy 143.51 22.86) (xy 143.51 26.67)))
  (wire (pts (xy 148.59 25.4) (xy 148.59 30.48)))
  (wire (pts (xy 90.17 113.03) (xy 91.44 113.03)))
  (wire (pts (xy 63.5 187.96) (xy 73.66 187.96)))
  (wire (pts (xy 208.28 147.32) (xy 205.74 147.32)))
  (wire (pts (xy 119.38 20.32) (xy 119.38 21.59)))
  (wire (pts (xy 135.89 172.72) (xy 135.89 171.45)))
  (wire (pts (xy 111.76 191.77) (xy 119.38 191.77)))
  (wire (pts (xy 49.53 107.95) (xy 50.8 107.95)))
  (wire (pts (xy 226.06 149.86) (xy 226.06 147.32)))
  (wire (pts (xy 252.73 46.99) (xy 252.73 49.53)))
  (wire (pts (xy 82.55 113.03) (xy 85.09 113.03)))
  (wire (pts (xy 205.74 144.78) (xy 205.74 147.32)))
  (wire (pts (xy 26.67 31.75) (xy 25.4 31.75)))
  (wire (pts (xy 63.5 172.72) (xy 73.66 172.72)))
  (wire (pts (xy 39.37 50.8) (xy 40.64 50.8)))
  (wire (pts (xy 27.94 107.95) (xy 41.91 107.95)))
  (wire (pts (xy 30.48 146.05) (xy 30.48 165.1)))
  (wire (pts (xy 252.73 49.53) (xy 255.27 49.53)))
  (wire (pts (xy 173.99 66.04) (xy 180.34 66.04)))
  (wire (pts (xy 82.55 106.68) (xy 82.55 113.03)))
  (wire (pts (xy 149.86 190.5) (xy 149.86 191.77)))
  (wire (pts (xy 226.06 154.94) (xy 226.06 152.4)))
  (wire (pts (xy 34.29 72.39) (xy 38.1 72.39)))
  (wire (pts (xy 173.99 40.64) (xy 180.34 40.64)))
  (wire (pts (xy 128.27 20.32) (xy 130.81 20.32)))
  (wire (pts (xy 149.86 184.15) (xy 157.48 184.15)))
  (wire (pts (xy 29.21 180.34) (xy 40.64 180.34)))
  (wire (pts (xy 173.99 119.38) (xy 180.34 119.38)))
  (wire (pts (xy 101.6 116.84) (xy 102.87 116.84)))
  (wire (pts (xy 274.32 58.42) (xy 274.32 60.96)))
  (wire (pts (xy 157.48 191.77) (xy 165.1 191.77)))
  (wire (pts (xy 252.73 49.53) (xy 252.73 52.07)))
  (wire (pts (xy 173.99 86.36) (xy 204.47 86.36)))
  (wire (pts (xy 91.44 119.38) (xy 85.09 119.38)))
  (wire (pts (xy 140.97 26.67) (xy 143.51 26.67)))
  (wire (pts (xy 114.3 172.72) (xy 114.3 171.45)))
  (wire (pts (xy 104.14 20.32) (xy 111.76 20.32)))
  (wire (pts (xy 111.76 27.94) (xy 119.38 27.94)))
  (wire (pts (xy 30.48 165.1) (xy 40.64 165.1)))
  (wire (pts (xy 173.99 111.76) (xy 180.34 111.76)))
  (wire (pts (xy 101.6 58.42) (xy 102.87 58.42)))
  (wire (pts (xy 173.99 73.66) (xy 180.34 73.66)))
  (wire (pts (xy 73.66 119.38) (xy 77.47 119.38)))
  (wire (pts (xy 228.6 154.94) (xy 226.06 154.94)))
  (wire (pts (xy 128.27 140.97) (xy 125.73 140.97)))
  (text "PB0 and PB1 should \nbe clamped to max \n3.3V input" (at 208.28 66.04 0))
  (text "Maximum current per output\npin is not to exceed 25 mA"
    (at 276.86 19.05 0)
  )
  (text "Maximum 15V on VIN. Not to be\nconnected while on USB power"
    (at 281.94 25.4 0)
  )
  (label "+USB_VBUS" (at 27.94 107.95 0) (fields_autoplaced))
  (label "D0(RX)" (at 73.66 190.5 180) (fields_autoplaced))
  (label "Q1G1" (at 265.43 120.65 0) (fields_autoplaced))
  (label "A0" (at 101.6 45.72 180) (fields_autoplaced))
  (label "D10" (at 101.6 63.5 180) (fields_autoplaced))
  (label "D7" (at 73.66 172.72 180) (fields_autoplaced))
  (label "A3" (at 101.6 38.1 180) (fields_autoplaced))
  (label "PB6(MISO)" (at 177.8 76.2 0) (fields_autoplaced))
  (label "D5" (at 73.66 177.8 180) (fields_autoplaced))
  (label "PF4" (at 101.6 66.04 180) (fields_autoplaced))
  (label "USB_D_P" (at 180.34 119.38 0) (fields_autoplaced))
  (label "Q1G1" (at 250.19 76.2 180) (fields_autoplaced))
  (label "OCS1" (at 101.6 86.36 180) (fields_autoplaced))
  (label "A5(SCL)" (at 180.34 66.04 0) (fields_autoplaced))
  (label "D13" (at 101.6 60.96 180) (fields_autoplaced))
  (label "XOSC_GND" (at 82.55 106.68 0) (fields_autoplaced))
  (label "PD7(U2TX)" (at 180.34 124.46 0) (fields_autoplaced))
  (label "D12" (at 101.6 55.88 180) (fields_autoplaced))
  (label "+AREF" (at 73.66 149.86 180) (fields_autoplaced))
  (label "~{RST}" (at 21.59 160.02 0) (fields_autoplaced))
  (label "D0(RX)" (at 180.34 38.1 0) (fields_autoplaced))
  (label "PB6_LED" (at 246.38 91.44 0) (fields_autoplaced))
  (label "~{WAKE}" (at 34.29 50.8 180) (fields_autoplaced))
  (label "Q1D2" (at 270.51 71.12 0) (fields_autoplaced))
  (label "10(SS)" (at 63.5 162.56 0) (fields_autoplaced))
  (label "D7" (at 180.34 73.66 0) (fields_autoplaced))
  (label "A2" (at 101.6 40.64 180) (fields_autoplaced))
  (label "PC7(U3TX)" (at 180.34 101.6 0) (fields_autoplaced))
  (label "D3" (at 73.66 182.88 180) (fields_autoplaced))
  (label "PC6(U3RX)" (at 180.34 99.06 0) (fields_autoplaced))
  (label "A4(SDA)" (at 73.66 147.32 180) (fields_autoplaced))
  (label "PB1(U1TX)" (at 50.8 107.95 0) (fields_autoplaced))
  (label "D8" (at 73.66 167.64 180) (fields_autoplaced))
  (label "A3" (at 29.21 185.42 0) (fields_autoplaced))
  (label "PA3" (at 180.34 45.72 0) (fields_autoplaced))
  (label "VIn" (at 34.29 74.93 180) (fields_autoplaced))
  (label "D8" (at 180.34 109.22 0) (fields_autoplaced))
  (label "VBAT" (at 101.6 116.84 180) (fields_autoplaced))
  (label "D1(TX)" (at 73.66 187.96 180) (fields_autoplaced))
  (label "D9" (at 73.66 165.1 180) (fields_autoplaced))
  (label "A5(SCL)" (at 29.21 190.5 0) (fields_autoplaced))
  (label "USB_ID" (at 29.21 118.11 0) (fields_autoplaced))
  (label "PC5(U4TX)" (at 180.34 96.52 0) (fields_autoplaced))
  (label "Q1G2" (at 270.51 76.2 0) (fields_autoplaced))
  (label "D6" (at 180.34 71.12 0) (fields_autoplaced))
  (label "PWR_LED" (at 265.43 52.07 0) (fields_autoplaced))
  (label "~{TARGET_RST}" (at 101.6 73.66 180) (fields_autoplaced))
  (label "D6" (at 73.66 175.26 180) (fields_autoplaced))
  (label "~{HIB}" (at 34.29 63.5 180) (fields_autoplaced))
  (label "+USB_VBUS" (at 34.29 72.39 180) (fields_autoplaced))
  (label "PC4(U4RX)" (at 180.34 93.98 0) (fields_autoplaced))
  (label "PB0(U1RX)" (at 50.8 118.11 0) (fields_autoplaced))
  (label "RX_LED" (at 265.43 44.45 0) (fields_autoplaced))
  (label "DEBUG_TCK" (at 180.34 83.82 0) (fields_autoplaced))
  (label "D12" (at 76.2 157.48 0) (fields_autoplaced))
  (label "IOREF" (at 138.43 161.29 0) (fields_autoplaced))
  (label "+USB_VBUS" (at 30.48 156.21 90) (fields_autoplaced))
  (label "VDDD" (at 135.89 26.67 0) (fields_autoplaced))
  (label "~{HIB}" (at 101.6 96.52 180) (fields_autoplaced))
  (label "PB6_LED" (at 265.43 49.53 0) (fields_autoplaced))
  (label "TX_LED" (at 265.43 46.99 0) (fields_autoplaced))
  (label "11(MOSI)" (at 63.5 160.02 0) (fields_autoplaced))
  (label "PD6(U2RX)" (at 180.34 121.92 0) (fields_autoplaced))
  (label "+USB_VBUS" (at 111.76 161.29 180) (fields_autoplaced))
  (label "PA4" (at 180.34 48.26 0) (fields_autoplaced))
  (label "~{TARGET_RST}" (at 50.8 31.75 0) (fields_autoplaced))
  (label "Q2D2" (at 270.51 99.06 0) (fields_autoplaced))
  (label "A4(SDA)" (at 180.34 68.58 0) (fields_autoplaced))
  (label "A5(SCL)" (at 180.34 111.76 0) (fields_autoplaced))
  (label "D2" (at 180.34 55.88 0) (fields_autoplaced))
  (label "TX_LED" (at 274.32 60.96 180) (fields_autoplaced))
  (label "D11" (at 76.2 160.02 0) (fields_autoplaced))
  (label "PA2" (at 180.34 43.18 0) (fields_autoplaced))
  (label "D0(RX)" (at 255.27 120.65 180) (fields_autoplaced))
  (label "D10" (at 76.2 162.56 0) (fields_autoplaced))
  (label "USB_D_P" (at 29.21 113.03 0) (fields_autoplaced))
  (label "-AREF" (at 146.05 137.16 0) (fields_autoplaced))
  (label "VIn" (at 29.21 172.72 0) (fields_autoplaced))
  (label "DEBUG_TDI" (at 180.34 88.9 0) (fields_autoplaced))
  (label "Q2G1" (at 265.43 125.73 0) (fields_autoplaced))
  (label "DEBUG_TDO" (at 180.34 91.44 0) (fields_autoplaced))
  (label "IOREF" (at 39.37 156.21 90) (fields_autoplaced))
  (label "Q2G1" (at 250.19 104.14 180) (fields_autoplaced))
  (label "13(SCK)" (at 63.5 154.94 0) (fields_autoplaced))
  (label "D1(TX)" (at 180.34 40.64 0) (fields_autoplaced))
  (label "A4(SDA)" (at 29.21 187.96 0) (fields_autoplaced))
  (label "XOSC_GND" (at 125.73 140.97 180) (fields_autoplaced))
  (label "12(MISO)" (at 63.5 157.48 0) (fields_autoplaced))
  (label "Q2D1" (at 247.65 99.06 0) (fields_autoplaced))
  (label "USB_D_N" (at 29.21 115.57 0) (fields_autoplaced))
  (label "XOSC1" (at 101.6 109.22 180) (fields_autoplaced))
  (label "VDDC" (at 120.65 20.32 0) (fields_autoplaced))
  (label "VBAT" (at 34.29 83.82 180) (fields_autoplaced))
  (label "USB_D_N" (at 180.34 116.84 0) (fields_autoplaced))
  (label "Q2G2" (at 265.43 128.27 0) (fields_autoplaced))
  (label "PB1(U1TX)" (at 180.34 63.5 0) (fields_autoplaced))
  (label "D4" (at 73.66 180.34 180) (fields_autoplaced))
  (label "A2" (at 29.21 182.88 0) (fields_autoplaced))
  (label "PB7(MOSI)" (at 177.8 78.74 0) (fields_autoplaced))
  (label "+AREF" (at 148.59 30.48 90) (fields_autoplaced))
  (label "D2" (at 73.66 185.42 180) (fields_autoplaced))
  (label "PA5" (at 180.34 50.8 0) (fields_autoplaced))
  (label "RX_LED" (at 246.38 60.96 0) (fields_autoplaced))
  (label "D9" (at 180.34 106.68 0) (fields_autoplaced))
  (label "A5(SCL)" (at 73.66 144.78 180) (fields_autoplaced))
  (label "A4(SDA)" (at 180.34 114.3 0) (fields_autoplaced))
  (label "D5" (at 101.6 50.8 180) (fields_autoplaced))
  (label "D1(TX)" (at 255.27 123.19 180) (fields_autoplaced))
  (label "~{RST}" (at 41.91 31.75 0) (fields_autoplaced))
  (label "Q1G2" (at 265.43 123.19 0) (fields_autoplaced))
  (label "A1" (at 29.21 180.34 0) (fields_autoplaced))
  (label "A0" (at 29.21 177.8 0) (fields_autoplaced))
  (label "PWR_LED" (at 274.32 91.44 180) (fields_autoplaced))
  (label "D4" (at 101.6 48.26 180) (fields_autoplaced))
  (label "PB6(MISO)" (at 255.27 125.73 180) (fields_autoplaced))
  (label "D3" (at 180.34 53.34 0) (fields_autoplaced))
  (label "DEBUG_TMS" (at 180.34 86.36 0) (fields_autoplaced))
  (label "OCS0" (at 101.6 81.28 180) (fields_autoplaced))
  (label "Q2G2" (at 270.51 104.14 0) (fields_autoplaced))
  (label "XOSC0" (at 101.6 104.14 180) (fields_autoplaced))
  (label "A1" (at 101.6 43.18 180) (fields_autoplaced))
  (label "D13" (at 76.2 154.94 0) (fields_autoplaced))
  (label "~{WAKE}" (at 101.6 93.98 180) (fields_autoplaced))
  (label "D11" (at 101.6 58.42 180) (fields_autoplaced))
  (label "Q1D1" (at 246.38 71.12 0) (fields_autoplaced))
  (label "PB0(U1RX)" (at 180.34 60.96 0) (fields_autoplaced))
  (symbol (lib_id "Roadrunner-rescue:USB_OTG") (at 20.32 113.03 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J1" (at 15.24 101.6 0))
    (property "Value" "USB_OTG" (at 15.24 104.14 0))
    (property "Footprint" "Connectors_USB_Local:USB_Micro_B_FCI_10118192" (at 24.13 114.3 0))
    (property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/FCI%20PDFs/10118192-0001LF_Webpage.PDF" (at 24.13 114.3 0))
    (property "Part #" "10118192-0001LF" (at 20.32 113.03 0))
    (property "Drawing" "http://portal.fciconnect.com/Comergent//fci/drawing/10118192.pdf" (at 20.32 113.03 0))
    (property "Description" "USB - micro B USB 2.0 Receptacle Connector 5 Position Surface Mount, Right Angle" (at 20.32 113.03 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (instances
      (project "Roadrunner"
        (path
          (reference "J1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:TM4C123GH6PM") (at 138.43 83.82 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U1" (at 106.68 33.02 0))
    (property "Value" "TM4C123GH6PM" (at 154.94 33.02 0))
    (property "Footprint" "Housings_QFP:LQFP-64_10x10mm_Pitch0.5mm" (at 138.43 83.82 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/tm4c123gh6pm.pdf" (at 138.43 78.74 0))
    (property "Description" "ARM® Cortex®-M4F Tiva™ C Microcontroller IC 32-Bit 80MHz 256KB (256K x 8) FLASH 64-LQFP (10x10)" (at 138.43 83.82 0))
    (property "Part #" "TM4C123GH6PMI7" (at 138.43 83.82 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "44")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
    (pin "5")
    (pin "50")
    (pin "51")
    (pin "52")
    (pin "53")
    (pin "54")
    (pin "55")
    (pin "56")
    (pin "57")
    (pin "58")
    (pin "59")
    (pin "6")
    (pin "60")
    (pin "61")
    (pin "62")
    (pin "63")
    (pin "64")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "Roadrunner"
        (path
          (reference "U1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:SW_PUSH") (at 30.48 31.75 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "SW1" (at 30.734 28.702 0))
    (property "Value" "RESET" (at 30.48 33.782 0))
    (property "Footprint" "Buttons_Switches_SMD_Local:SW_SPST_WS-TASV_4.5x4.5mm" (at 30.48 31.75 0))
    (property "Datasheet" "http://katalog.we-online.de/em/datasheet/430181038816.pdf" (at 30.48 31.75 0))
    (property "Part #" "430181038816" (at 30.48 31.75 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "SW1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:R") (at 38.1 26.67 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R1" (at 40.132 26.67 90))
    (property "Value" "10k" (at 38.1 26.67 90))
    (property "Footprint" "Resistors_SMD:R_0603_HandSoldering" (at 36.322 26.67 90))
    (property "Datasheet" "http://www.yageo.com/pdf/Pu-RC0603_51_PbFree_L_2.pdf" (at 38.1 26.67 0))
    (property "Description" "10k Ohm ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film" (at 38.1 26.67 90))
    (property "Part #" "RC0603FR-0710KL" (at 38.1 26.67 90))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "R1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:+3.3V") (at 38.1 20.32 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR01" (at 38.1 24.13 0))
    (property "Value" "+3.3V" (at 38.1 16.764 0))
    (property "Footprint" "" (at 38.1 20.32 0))
    (property "Datasheet" "" (at 38.1 20.32 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR01") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:HEADER_1") (at 46.99 26.67 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J3" (at 46.99 25.4 0))
    (property "Value" "~RST" (at 44.45 25.4 0))
    (property "Footprint" "Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm" (at 46.99 26.67 0))
    (property "Datasheet" "" (at 46.99 26.67 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "J3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:Crystal") (at 81.28 119.38 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "Y1" (at 81.28 115.57 0))
    (property "Value" "32.768Khz" (at 81.28 123.19 0))
    (property "Footprint" "Project-Symbols_Local:Crystal_C26-LF_d2.1mm_l6.5mm_Horizontal_1EP_style1" (at 81.28 119.38 0))
    (property "Datasheet" "http://cfd.citizen.co.jp/english/prod-tech/product/pdf/datasheet_TF/CFS-145%20CFS-206%20CFV-206_E.pdf" (at 81.28 119.38 0))
    (property "Part #" "CFS-20632768HZFB" (at 81.28 119.38 0))
    (property "Description" "32.768kHz ±5ppm Crystal 12.5pF 35 kOhm -20°C ~ 70°C Through Hole Cylindrical Can, Radial" (at 81.28 119.38 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "Y1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:C_Small") (at 77.47 113.03 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C1" (at 75.692 112.776 0))
    (property "Value" "24pF" (at 79.502 112.776 0))
    (property "Footprint" "Capacitors_SMD:C_0603" (at 77.47 113.03 0))
    (property "Datasheet" "http://www.yageo.com/documents/recent/UPY-GP_NP0_16V-to-50V_16.pdf" (at 77.47 113.03 0))
    (property "Description" "24pF ±5% 50V Ceramic Capacitor C0G, NP0 0603" (at 77.47 113.03 0))
    (property "Part #" "CC0603JRNPO9BN240" (at 77.47 113.03 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:GNDREF") (at 76.2 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR02" (at 76.2 100.33 0))
    (property "Value" "GNDREF" (at 76.2 97.79 0))
    (property "Footprint" "" (at 76.2 93.98 0))
    (property "Datasheet" "" (at 76.2 93.98 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR02") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:GNDREF") (at 88.9 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR03" (at 88.9 100.33 0))
    (property "Value" "GNDREF" (at 88.9 97.79 0))
    (property "Footprint" "" (at 88.9 93.98 0))
    (property "Datasheet" "" (at 88.9 93.98 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR03") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:C_Small") (at 88.9 90.17 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C4" (at 89.154 88.392 0))
    (property "Value" "10pF" (at 89.154 92.202 0))
    (property "Footprint" "Capacitors_SMD:C_0603" (at 88.9 90.17 0))
    (property "Datasheet" "https://www.digikey.com/catalog/en/partgroup/c0g-np0-dielectric-commercial-grade/3830?mpart=C0603C100J5GACTU&vendor=399" (at 88.9 90.17 0))
    (property "Description" "CAP CER 10PF 50V C0G/NP0 0603" (at 88.9 90.17 0))
    (property "Part #" "C0603C100J5GACTU" (at 88.9 90.17 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:C_Small") (at 76.2 90.17 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C3" (at 76.454 88.392 0))
    (property "Value" "10pF" (at 76.454 92.202 0))
    (property "Footprint" "Capacitors_SMD:C_0603" (at 76.2 90.17 0))
    (property "Datasheet" "https://www.digikey.com/catalog/en/partgroup/c0g-np0-dielectric-commercial-grade/3830?mpart=C0603C100J5GACTU&vendor=399" (at 76.2 90.17 0))
    (property "Description" "CAP CER 10PF 50V C0G/NP0 0603" (at 76.2 90.17 0))
    (property "Part #" "C0603C100J5GACTU" (at 76.2 90.17 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:Crystal") (at 83.82 86.36 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "Y2" (at 83.82 82.55 0))
    (property "Value" "16MHz" (at 83.82 90.17 0))
    (property "Footprint" "Crystals:Crystal_SMD_5032-2pin_5.0x3.2mm_HandSoldering" (at 83.82 86.36 0))
    (property "Datasheet" "http://www.ndk.com/images/products/catalog/c_NX5032GA_e.pdf" (at 83.82 86.36 0))
    (property "Part #" "NX5032GA-16MHZ-STD-CSK-4" (at 83.82 86.36 0))
    (property "Description" "16MHz ±20ppm Crystal 8pF 50 Ohm -10°C ~ 70°C Surface Mount 2-SMD, No Lead" (at 83.82 86.36 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "Y2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:GNDREF") (at 25.4 33.02 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR04" (at 25.4 39.37 0))
    (property "Value" "GNDREF" (at 25.4 36.83 0))
    (property "Footprint" "" (at 25.4 33.02 0))
    (property "Datasheet" "" (at 25.4 33.02 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR04") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:GNDREF") (at 20.32 125.73 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR05" (at 20.32 132.08 0))
    (property "Value" "GNDREF" (at 20.32 129.54 0))
    (property "Footprint" "" (at 20.32 125.73 0))
    (property "Datasheet" "" (at 20.32 125.73 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR05") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:GNDREF") (at 140.97 144.78 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR06" (at 140.97 151.13 0))
    (property "Value" "GNDREF" (at 140.97 148.59 0))
    (property "Footprint" "" (at 140.97 144.78 0))
    (property "Datasheet" "" (at 140.97 144.78 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR06") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:+3.3V") (at 143.51 22.86 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR07" (at 143.51 26.67 0))
    (property "Value" "+3.3V" (at 143.51 19.304 0))
    (property "Footprint" "" (at 143.51 22.86 0))
    (property "Datasheet" "" (at 143.51 22.86 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR07") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:C_Small") (at 111.76 187.96 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C5" (at 112.014 186.182 0))
    (property "Value" "0.1uF" (at 112.014 189.992 0))
    (property "Footprint" "Capacitors_SMD:C_0603" (at 111.76 187.96 0))
    (property "Datasheet" "http://www.yageo.com/documents/recent/UPY-GPHC_X7R_6.3V-to-50V_17.pdf" (at 111.76 187.96 0))
    (property "Description" "6.3 V to 25 V, X5R/X7R ceramic chip" (at 111.76 187.96 0))
    (property "Part #" "CC0603JRX7R8BB104" (at 111.76 187.96 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:C_Small") (at 119.38 187.96 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C6" (at 119.634 186.182 0))
    (property "Value" "22.0uF" (at 119.634 189.992 0))
    (property "Footprint" "Capacitors_SMD:C_0805" (at 119.38 187.96 0))
    (property "Datasheet" "http://www.samsungsem.com/kr/support/library/product-catalog/__icsFiles/afieldfile/2016/09/27/MLCC.pdf" (at 119.38 187.96 0))
    (property "Description" "6.3 V to 25 V, X5R/X7R ceramic chip" (at 119.38 187.96 0))
    (property "Part #" "CL21A226MOCLRNC" (at 119.38 187.96 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C6") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:C_Small") (at 127 187.96 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C7" (at 127.254 186.182 0))
    (property "Value" "0.1uF" (at 127.254 189.992 0))
    (property "Footprint" "Capacitors_SMD:C_0603" (at 127 187.96 0))
    (property "Datasheet" "" (at 127 187.96 0))
    (property "Description" "6.3 V to 25 V, X5R/X7R ceramic chip" (at 127 187.96 0))
    (property "Part #" "CC0603JRX7R8BB104" (at 127 187.96 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C7") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:C_Small") (at 134.62 187.96 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C8" (at 134.874 186.182 0))
    (property "Value" "22.0uF" (at 134.874 189.992 0))
    (property "Footprint" "Capacitors_SMD:C_0805" (at 134.62 187.96 0))
    (property "Datasheet" "" (at 134.62 187.96 0))
    (property "Description" "6.3 V to 25 V, X5R/X7R ceramic chip" (at 134.62 187.96 0))
    (property "Part #" "CL21A226MOCLRNC" (at 134.62 187.96 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C8") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:C_Small") (at 142.24 187.96 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C9" (at 142.494 186.182 0))
    (property "Value" "0.1uF" (at 142.494 189.992 0))
    (property "Footprint" "Capacitors_SMD:C_0603" (at 142.24 187.96 0))
    (property "Datasheet" "" (at 142.24 187.96 0))
    (property "Description" "6.3 V to 25 V, X5R/X7R ceramic chip" (at 142.24 187.96 0))
    (property "Part #" "CC0603JRX7R8BB104" (at 142.24 187.96 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C9") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:C_Small") (at 149.86 187.96 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C10" (at 150.114 186.182 0))
    (property "Value" "22.0uF" (at 150.114 189.992 0))
    (property "Footprint" "Capacitors_SMD:C_0805" (at 149.86 187.96 0))
    (property "Datasheet" "" (at 149.86 187.96 0))
    (property "Description" "6.3 V to 25 V, X5R/X7R ceramic chip" (at 149.86 187.96 0))
    (property "Part #" "CL21A226MOCLRNC" (at 149.86 187.96 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C10") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:GNDREF") (at 149.86 193.04 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR017" (at 149.86 199.39 0))
    (property "Value" "GNDREF" (at 149.86 196.85 0))
    (property "Footprint" "" (at 149.86 193.04 0))
    (property "Datasheet" "" (at 149.86 193.04 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR017") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:R") (at 44.45 50.8 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R2" (at 44.45 52.832 90))
    (property "Value" "1M" (at 44.45 50.8 90))
    (property "Footprint" "Resistors_SMD:R_0603_HandSoldering" (at 44.45 49.022 90))
    (property "Datasheet" "http://www.vishay.com/docs/20047/rcge3.pdf" (at 44.45 50.8 0))
    (property "Description" "1M Ohm ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film" (at 44.45 50.8 90))
    (property "Part #" "RCG06031M00FKEA" (at 44.45 50.8 90))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "R2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:+3.3V") (at 50.8 48.26 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR08" (at 50.8 52.07 0))
    (property "Value" "+3.3V" (at 50.8 44.704 0))
    (property "Footprint" "" (at 50.8 48.26 0))
    (property "Datasheet" "" (at 50.8 48.26 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR08") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:+3.3V") (at 135.89 157.48 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR09" (at 135.89 161.29 0))
    (property "Value" "+3.3V" (at 135.89 153.924 0))
    (property "Footprint" "" (at 135.89 157.48 0))
    (property "Datasheet" "" (at 135.89 157.48 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR09") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:HEADER_1") (at 40.64 63.5 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J5" (at 41.91 63.5 0))
    (property "Value" "~HIB" (at 41.91 60.96 0))
    (property "Footprint" "Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm" (at 40.64 63.5 0))
    (property "Datasheet" "" (at 40.64 63.5 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "J5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:C_Small") (at 119.38 24.13 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C14" (at 119.634 22.352 0))
    (property "Value" "0.1uF" (at 119.634 26.162 0))
    (property "Footprint" "Capacitors_SMD:C_0603" (at 119.38 24.13 0))
    (property "Datasheet" "http://www.yageo.com/documents/recent/UPY-GPHC_X7R_6.3V-to-50V_17.pdf" (at 119.38 24.13 0))
    (property "Part #" "CC0603JRX7R8BB104" (at 119.38 24.13 0))
    (property "Description" "CAP CER 0.1UF 25V X7R 0603" (at 119.38 24.13 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C14") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:C_Small") (at 111.76 24.13 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C13" (at 112.014 22.352 0))
    (property "Value" "1.0uF" (at 112.014 26.162 0))
    (property "Footprint" "Capacitors_SMD:C_0603" (at 111.76 24.13 0))
    (property "Datasheet" "http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM188R61C105KA93-01.pdf" (at 111.76 24.13 0))
    (property "Part #" "GRM188R61C105KA93D" (at 111.76 24.13 0))
    (property "Description" "CAP CER 1UF 16V X5R 0603" (at 111.76 24.13 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C13") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:C_Small") (at 104.14 24.13 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C12" (at 104.394 22.352 0))
    (property "Value" "2.2uF" (at 104.394 26.162 0))
    (property "Footprint" "Capacitors_SMD:C_0603" (at 104.14 24.13 0))
    (property "Datasheet" "http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM188R61C225KE15-01.pdf" (at 104.14 24.13 0))
    (property "Part #" "GRM188R61C225KE15D" (at 104.14 24.13 0))
    (property "Description" "CAP CER 2.2UF 16V X5R 0603" (at 104.14 24.13 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C12") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:GNDREF") (at 119.38 29.21 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR010" (at 119.38 35.56 0))
    (property "Value" "GNDREF" (at 119.38 33.02 0))
    (property "Footprint" "" (at 119.38 29.21 0))
    (property "Datasheet" "" (at 119.38 29.21 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR010") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X08") (at 45.72 163.83 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J7" (at 45.72 152.4 0))
    (property "Value" "Power" (at 48.26 163.83 90))
    (property "Footprint" "Socket_Strips:Socket_Strip_Straight_1x08_Pitch2.54mm" (at 45.72 163.83 0))
    (property "Datasheet" "" (at 45.72 163.83 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (instances
      (project "Roadrunner"
        (path
          (reference "J7") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X06") (at 45.72 184.15 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J8" (at 45.72 175.26 0))
    (property "Value" "Analog" (at 48.26 184.15 90))
    (property "Footprint" "Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm" (at 45.72 184.15 0))
    (property "Datasheet" "" (at 45.72 184.15 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (instances
      (project "Roadrunner"
        (path
          (reference "J8") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X10") (at 58.42 156.21 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J9" (at 58.42 142.24 0))
    (property "Value" "Digital" (at 55.88 156.21 90))
    (property "Footprint" "Socket_Strips:Socket_Strip_Straight_1x10_Pitch2.54mm" (at 58.42 156.21 0))
    (property "Datasheet" "" (at 58.42 156.21 0))
    (pin "1")
    (pin "10")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "Roadrunner"
        (path
          (reference "J9") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X08") (at 58.42 181.61 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J10" (at 58.42 170.18 0))
    (property "Value" "Digital" (at 55.88 181.61 90))
    (property "Footprint" "Socket_Strips:Socket_Strip_Straight_1x08_Pitch2.54mm" (at 58.42 181.61 0))
    (property "Datasheet" "" (at 58.42 181.61 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (instances
      (project "Roadrunner"
        (path
          (reference "J10") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:GNDREF") (at 85.09 153.67 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR011" (at 85.09 160.02 0))
    (property "Value" "GNDREF" (at 85.09 157.48 0))
    (property "Footprint" "" (at 85.09 153.67 0))
    (property "Datasheet" "" (at 85.09 153.67 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR011") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:GNDREF") (at 36.83 167.64 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR012" (at 36.83 173.99 0))
    (property "Value" "GNDREF" (at 36.83 171.45 0))
    (property "Footprint" "" (at 36.83 167.64 0))
    (property "Datasheet" "" (at 36.83 167.64 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR012") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:+3.3V") (at 34.29 149.86 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR013" (at 34.29 153.67 0))
    (property "Value" "+3.3V" (at 34.29 146.304 0))
    (property "Footprint" "" (at 34.29 149.86 0))
    (property "Datasheet" "" (at 34.29 149.86 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR013") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:+5V") (at 30.48 146.05 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR014" (at 30.48 149.86 0))
    (property "Value" "+5V" (at 30.48 142.494 0))
    (property "Footprint" "" (at 30.48 146.05 0))
    (property "Datasheet" "" (at 30.48 146.05 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR014") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:+3.3V") (at 149.86 182.88 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR015" (at 149.86 186.69 0))
    (property "Value" "+3.3V" (at 149.86 179.324 0))
    (property "Footprint" "" (at 149.86 182.88 0))
    (property "Datasheet" "" (at 149.86 182.88 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR015") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X02") (at 153.67 24.13 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J16" (at 153.67 27.94 0))
    (property "Value" "+AREF" (at 156.21 24.13 90))
    (property "Footprint" "Custom-Mounting-Holes:NetTie-I_Connected_SMD" (at 153.67 24.13 0))
    (property "Datasheet" "" (at 153.67 24.13 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "J16") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X02") (at 151.13 142.24 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J15" (at 151.13 138.43 0))
    (property "Value" "-AREF" (at 153.67 142.24 90))
    (property "Footprint" "Custom-Mounting-Holes:NetTie-I_Connected_SMD" (at 151.13 142.24 0))
    (property "Datasheet" "" (at 151.13 142.24 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "J15") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X04") (at 203.2 46.99 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J20" (at 203.2 40.64 0))
    (property "Value" "SPI 0" (at 205.74 46.99 90))
    (property "Footprint" "Socket_Strips:Socket_Strip_Straight_2x02_Pitch2.54mm" (at 203.2 46.99 0))
    (property "Datasheet" "" (at 203.2 46.99 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (instances
      (project "Roadrunner"
        (path
          (reference "J20") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X02") (at 203.2 62.23 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J21" (at 203.2 58.42 0))
    (property "Value" "SERIAL 1" (at 205.74 62.23 90))
    (property "Footprint" "Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm" (at 203.2 62.23 0))
    (property "Datasheet" "" (at 203.2 62.23 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "J21") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X02") (at 201.93 123.19 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J19" (at 201.93 119.38 0))
    (property "Value" "SERIAL 2" (at 204.47 123.19 90))
    (property "Footprint" "Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm" (at 201.93 123.19 0))
    (property "Datasheet" "" (at 201.93 123.19 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "J19") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X01") (at 91.44 66.04 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J4" (at 91.44 68.58 0))
    (property "Value" "PF4" (at 88.9 66.04 90))
    (property "Footprint" "Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm" (at 91.44 66.04 0))
    (property "Datasheet" "" (at 91.44 66.04 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "J4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X02") (at 203.2 77.47 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J17" (at 203.2 73.66 0))
    (property "Value" "SPI 2 (D22,D23)" (at 205.74 77.47 90))
    (property "Footprint" "Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm" (at 203.2 77.47 0))
    (property "Datasheet" "" (at 203.2 77.47 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "J17") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:C_Small") (at 165.1 187.96 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C16" (at 165.354 186.182 0))
    (property "Value" "22.0uF" (at 165.354 189.992 0))
    (property "Footprint" "Capacitors_SMD:C_0805" (at 165.1 187.96 0))
    (property "Datasheet" "" (at 165.1 187.96 0))
    (property "Description" "6.3 V to 25 V, X5R/X7R ceramic chip" (at 165.1 187.96 0))
    (property "Part #" "CL21A226MOCLRNC" (at 165.1 187.96 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C16") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:C_Small") (at 157.48 187.96 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C15" (at 157.734 186.182 0))
    (property "Value" "0.1uF" (at 157.734 189.992 0))
    (property "Footprint" "Capacitors_SMD:C_0603" (at 157.48 187.96 0))
    (property "Datasheet" "" (at 157.48 187.96 0))
    (property "Description" "6.3 V to 25 V, X5R/X7R ceramic chip" (at 157.48 187.96 0))
    (property "Part #" "CC0603JRX7R8BB104" (at 157.48 187.96 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C15") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:R") (at 45.72 118.11 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R5" (at 45.72 116.078 90))
    (property "Value" "R" (at 45.72 118.11 90))
    (property "Footprint" "Resistors_SMD:R_0805_HandSoldering" (at 45.72 119.888 90))
    (property "Datasheet" "" (at 45.72 118.11 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "R5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:R") (at 45.72 107.95 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R6" (at 45.72 105.918 90))
    (property "Value" "R" (at 45.72 107.95 90))
    (property "Footprint" "Resistors_SMD:R_0805_HandSoldering" (at 45.72 109.728 90))
    (property "Datasheet" "" (at 45.72 107.95 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "R6") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CP") (at 135.89 167.64 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C17" (at 136.525 165.1 0))
    (property "Value" "22.0uF" (at 136.525 170.18 0))
    (property "Footprint" "Capacitors_Tantalum_SMD:CP_Tantalum_Case-C_EIA-6032-28_Hand" (at 136.8552 171.45 0))
    (property "Datasheet" "http://www.kemet.com/Lists/ProductCatalog/Attachments/254/KEM_T2005_T491.pdf" (at 135.89 167.64 0))
    (property "Description" "22µF ±10% Molded Tantalum Capacitors 16V 2413 (6032 Metric) 1.6 Ohm" (at 135.89 167.64 0))
    (property "Part #" "T491C226K016AT" (at 135.89 167.64 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C17") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:GNDREF") (at 125.73 173.99 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR016" (at 125.73 180.34 0))
    (property "Value" "GNDREF" (at 125.73 177.8 0))
    (property "Footprint" "" (at 125.73 173.99 0))
    (property "Datasheet" "" (at 125.73 173.99 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR016") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CP") (at 114.3 167.64 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C11" (at 114.935 165.1 0))
    (property "Value" "10.0uF" (at 114.935 170.18 0))
    (property "Footprint" "Capacitors_SMD:C_0805" (at 115.2652 171.45 0))
    (property "Datasheet" "" (at 114.3 167.64 0))
    (property "Type" "Tantalum" (at 114.3 167.64 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C11") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:LM1117-3.3") (at 125.73 161.29 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U2" (at 128.27 167.64 0))
    (property "Value" "LM1117-3.3" (at 125.73 154.94 0))
    (property "Footprint" "TO_SOT_Packages_SMD:SOT-223" (at 125.73 161.29 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf" (at 125.73 161.29 0))
    (property "Description" "Linear Voltage Regulator IC Positive Fixed Output 3.3V 800mA SOT-223-4" (at 125.73 161.29 0))
    (property "Part #" "LM1117IMPX-3.3/NOPB" (at 125.73 161.29 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (instances
      (project "Roadrunner"
        (path
          (reference "U2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:LED_ALT") (at 246.38 64.77 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "D3" (at 243.84 64.77 0))
    (property "Value" "Green" (at 248.92 64.77 0))
    (property "Footprint" "LEDs:LED_0805" (at 246.38 64.77 0))
    (property "Datasheet" "http://www.osram-os.com/Graphics/XPic9/00078860_0.pdf" (at 246.38 64.77 0))
    (property "Current " "20mA" (at 246.38 64.77 0))
    (property "Description" "Green 570nm LED Indication - Discrete 2.2V 0805 (2012 Metric)" (at 246.38 64.77 0))
    (property "Part #" "LG R971-KN-1" (at 246.38 64.77 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "D3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:GNDREF") (at 271.78 81.28 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR018" (at 271.78 87.63 0))
    (property "Value" "GNDREF" (at 271.78 85.09 0))
    (property "Footprint" "" (at 271.78 81.28 0))
    (property "Datasheet" "" (at 271.78 81.28 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR018") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:LED_ALT") (at 274.32 64.77 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "D2" (at 271.78 64.77 0))
    (property "Value" "Green" (at 276.86 64.77 0))
    (property "Footprint" "LEDs:LED_0805" (at 274.32 64.77 0))
    (property "Datasheet" "http://www.osram-os.com/Graphics/XPic9/00078860_0.pdf" (at 274.32 64.77 0))
    (property "Current " "20mA" (at 274.32 64.77 0))
    (property "Description" "Green 570nm LED Indication - Discrete 2.2V 0805 (2012 Metric)" (at 274.32 64.77 0))
    (property "Part #" "LG R971-KN-1" (at 274.32 64.77 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "D2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:GNDREF") (at 248.92 81.28 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR019" (at 248.92 87.63 0))
    (property "Value" "GNDREF" (at 248.92 85.09 0))
    (property "Footprint" "" (at 248.92 81.28 0))
    (property "Datasheet" "" (at 248.92 81.28 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR019") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:M_Hole") (at 255.27 149.86 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "T1" (at 255.27 147.32 0))
    (property "Value" "M_Hole" (at 255.27 144.78 0))
    (property "Footprint" "Custom-Mounting-Holes:ArduinoMountingHole_3.2mm" (at 255.27 149.86 0))
    (property "Datasheet" "" (at 255.27 149.86 0))
    (instances
      (project "Roadrunner"
        (path
          (reference "T1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:M_Hole") (at 265.43 149.86 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "T3" (at 265.43 147.32 0))
    (property "Value" "M_Hole" (at 265.43 144.78 0))
    (property "Footprint" "Custom-Mounting-Holes:ArduinoMountingHole_3.2mm" (at 265.43 149.86 0))
    (property "Datasheet" "" (at 265.43 149.86 0))
    (instances
      (project "Roadrunner"
        (path
          (reference "T3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:M_Hole") (at 255.27 158.75 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "T2" (at 255.27 156.21 0))
    (property "Value" "M_Hole" (at 255.27 153.67 0))
    (property "Footprint" "Custom-Mounting-Holes:ArduinoMountingHole_3.2mm" (at 255.27 158.75 0))
    (property "Datasheet" "" (at 255.27 158.75 0))
    (instances
      (project "Roadrunner"
        (path
          (reference "T2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:M_Hole") (at 265.43 158.75 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "T4" (at 265.43 156.21 0))
    (property "Value" "M_Hole" (at 265.43 153.67 0))
    (property "Footprint" "Custom-Mounting-Holes:ArduinoMountingHole_3.2mm" (at 265.43 158.75 0))
    (property "Datasheet" "" (at 265.43 158.75 0))
    (instances
      (project "Roadrunner"
        (path
          (reference "T4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X02") (at 201.93 100.33 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J14" (at 213.36 100.33 0))
    (property "Value" "SERIAL 3" (at 203.2 100.33 0))
    (property "Footprint" "Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm" (at 201.93 100.33 0))
    (property "Datasheet" "" (at 201.93 100.33 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "J14") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X02") (at 201.93 95.25 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J13" (at 213.36 95.25 0))
    (property "Value" "SERIAL 4" (at 203.2 95.25 0))
    (property "Footprint" "Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm" (at 201.93 95.25 0))
    (property "Datasheet" "" (at 201.93 95.25 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "J13") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X04") (at 209.55 87.63 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J2" (at 209.55 81.28 0))
    (property "Value" "JTAG" (at 212.09 87.63 90))
    (property "Footprint" "Pin_Headers:Pin_Header_Straight_2x02_Pitch2.54mm" (at 209.55 87.63 0))
    (property "Datasheet" "" (at 209.55 87.63 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (instances
      (project "Roadrunner"
        (path
          (reference "J2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:LED_ALT") (at 246.38 95.25 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "D4" (at 243.84 95.25 0))
    (property "Value" "Green" (at 248.92 95.25 0))
    (property "Footprint" "LEDs:LED_0805" (at 246.38 95.25 0))
    (property "Datasheet" "http://www.osram-os.com/Graphics/XPic9/00078860_0.pdf" (at 246.38 95.25 0))
    (property "Current " "20mA" (at 246.38 95.25 0))
    (property "Description" "Green 570nm LED Indication - Discrete 2.2V 0805 (2012 Metric)" (at 246.38 95.25 0))
    (property "Part #" "LG R971-KN-1" (at 246.38 95.25 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "D4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:GNDREF") (at 271.78 109.22 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR020" (at 271.78 115.57 0))
    (property "Value" "GNDREF" (at 271.78 113.03 0))
    (property "Footprint" "" (at 271.78 109.22 0))
    (property "Datasheet" "" (at 271.78 109.22 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR020") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:LED_ALT") (at 274.32 95.25 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "D5" (at 271.78 95.25 0))
    (property "Value" "Green" (at 276.86 95.25 0))
    (property "Footprint" "LEDs:LED_0805" (at 274.32 95.25 0))
    (property "Datasheet" "http://www.osram-os.com/Graphics/XPic9/00078860_0.pdf" (at 274.32 95.25 0))
    (property "Current " "20mA" (at 274.32 95.25 0))
    (property "Description" "Green 570nm LED Indication - Discrete 2.2V 0805 (2012 Metric)" (at 274.32 95.25 0))
    (property "Part #" "LG R971-KN-1" (at 274.32 95.25 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "D5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:GNDREF") (at 248.92 109.22 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR021" (at 248.92 115.57 0))
    (property "Value" "GNDREF" (at 248.92 113.03 0))
    (property "Footprint" "" (at 248.92 109.22 0))
    (property "Datasheet" "" (at 248.92 109.22 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR021") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:UM6K33N") (at 260.35 104.14 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "Q2" (at 255.27 93.345 0))
    (property "Value" "UM6K33N" (at 255.27 95.25 0))
    (property "Footprint" "TO_SOT_Packages_SMD:SOT-363_SC-70-6" (at 255.27 97.155 0))
    (property "Datasheet" "http://www.rohm.com/web/global/datasheet/UM6K33N/um6k33n-e" (at 265.43 88.9 0))
    (property "Part #" "UM6K33NTN" (at 260.35 104.14 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (instances
      (project "Roadrunner"
        (path
          (reference "Q2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:UM6K33N") (at 260.35 76.2 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "Q1" (at 255.27 65.405 0))
    (property "Value" "UM6K33N" (at 255.27 67.31 0))
    (property "Footprint" "TO_SOT_Packages_SMD:SOT-363_SC-70-6" (at 255.27 69.215 0))
    (property "Datasheet" "http://www.rohm.com/web/global/datasheet/UM6K33N/um6k33n-e" (at 265.43 60.96 0))
    (property "Part #" "UM6K33NTN" (at 260.35 76.2 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (instances
      (project "Roadrunner"
        (path
          (reference "Q1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:R_Pack04") (at 260.35 125.73 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "RN2" (at 260.35 118.11 90))
    (property "Value" "10k" (at 260.35 130.81 90))
    (property "Footprint" "Project-Symbols_Local:YC164-JR-0775RL" (at 260.35 132.715 90))
    (property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Panasonic%20Resistors%20Thermistors%20PDFs/EXB38V%20Spec.pdf" (at 260.35 125.73 0))
    (property "Part #" "EXB-38V103JV" (at 260.35 125.73 90))
    (property "Description" "RES ARRAY 4 RES 10K OHM 1206" (at 260.35 125.73 90))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (instances
      (project "Roadrunner"
        (path
          (reference "RN2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:R_Pack04") (at 260.35 49.53 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "RN1" (at 260.35 41.91 90))
    (property "Value" "75" (at 260.35 54.61 90))
    (property "Footprint" "Project-Symbols_Local:YC164-JR-0775RL" (at 260.35 56.515 90))
    (property "Datasheet" "http://media.digikey.com/pdf/Data%20Sheets/Yageo%20PDFs/YC102-358,TC122-164_Series_DS.pdf" (at 260.35 49.53 0))
    (property "Part #" "YC164-JR-0775RL" (at 260.35 49.53 90))
    (property "Description" "RES ARRAY 4 RES 75 OHM 1206" (at 260.35 49.53 90))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (instances
      (project "Roadrunner"
        (path
          (reference "RN1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:+3.3V") (at 252.73 43.18 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR022" (at 252.73 46.99 0))
    (property "Value" "+3.3V" (at 252.73 39.624 0))
    (property "Footprint" "" (at 252.73 43.18 0))
    (property "Datasheet" "" (at 252.73 43.18 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR022") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:+3.3V") (at 255.27 128.27 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR023" (at 259.08 128.27 0))
    (property "Value" "+3.3V" (at 251.714 128.27 0))
    (property "Footprint" "" (at 255.27 128.27 0))
    (property "Datasheet" "" (at 255.27 128.27 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR023") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:+3.3V") (at 41.91 83.82 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR024" (at 41.91 87.63 0))
    (property "Value" "+3.3V" (at 41.91 80.264 0))
    (property "Footprint" "" (at 41.91 83.82 0))
    (property "Datasheet" "" (at 41.91 83.82 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR024") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:HEADER_1") (at 39.37 46.99 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J11" (at 39.37 45.72 0))
    (property "Value" "~WAKE" (at 36.83 45.72 0))
    (property "Footprint" "Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm" (at 39.37 46.99 0))
    (property "Datasheet" "" (at 39.37 46.99 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "J11") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X02") (at 43.18 73.66 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J6" (at 43.18 77.47 0))
    (property "Value" "VIn" (at 45.72 73.66 90))
    (property "Footprint" "Custom-Mounting-Holes:NetTie-I_Connected_SMD" (at 43.18 73.66 0))
    (property "Datasheet" "" (at 43.18 73.66 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "J6") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:C_Small") (at 87.63 113.03 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C2" (at 85.852 112.776 0))
    (property "Value" "24pF" (at 89.662 112.776 0))
    (property "Footprint" "Capacitors_SMD:C_0603" (at 87.63 113.03 0))
    (property "Datasheet" "http://www.yageo.com/documents/recent/UPY-GP_NP0_16V-to-50V_16.pdf" (at 87.63 113.03 0))
    (property "Description" "24pF ±5% 50V Ceramic Capacitor C0G, NP0 0603" (at 87.63 113.03 0))
    (property "Part #" "CC0603JRNPO9BN240" (at 87.63 113.03 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Roadrunner"
        (path
          (reference "C2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X04") (at 213.36 151.13 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J12" (at 213.36 144.78 0))
    (property "Value" "Power" (at 215.9 151.13 90))
    (property "Footprint" "Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm" (at 213.36 151.13 0))
    (property "Datasheet" "" (at 213.36 151.13 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (instances
      (project "Roadrunner"
        (path
          (reference "J12") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:CONN_01X04") (at 233.68 151.13 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J18" (at 233.68 144.78 0))
    (property "Value" "Ground" (at 236.22 151.13 90))
    (property "Footprint" "Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm" (at 233.68 151.13 0))
    (property "Datasheet" "" (at 233.68 151.13 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (instances
      (project "Roadrunner"
        (path
          (reference "J18") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:GNDREF") (at 226.06 157.48 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR025" (at 226.06 163.83 0))
    (property "Value" "GNDREF" (at 226.06 161.29 0))
    (property "Footprint" "" (at 226.06 157.48 0))
    (property "Datasheet" "" (at 226.06 157.48 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR025") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Roadrunner-rescue:+3.3V") (at 205.74 144.78 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR026" (at 205.74 148.59 0))
    (property "Value" "+3.3V" (at 205.74 141.224 0))
    (property "Footprint" "" (at 205.74 144.78 0))
    (property "Datasheet" "" (at 205.74 144.78 0))
    (pin "1")
    (instances
      (project "Roadrunner"
        (path
          (reference "#PWR026") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
