PB Docking Update: 6 October, 2011

1. Still planning on conducting Test 2 during the week of October 17th
2. AUV 
a. Daphne will be in the tank early next week.  Docking payload is calibrated, integrated and operational.
3. Dock
a. Next test uses the acoustic modem hanging on a hand deployed mooring
b. Mock Dock
i. Mooring
1. Scrambling to find an armored cable solution for the buoy to subsea float.
a. Probably uses Non-CAT5 cable: 2-wire Ethernet
i. Enable-IT Ethernet extender (~8W!)
ii. Patton, or other DSL type
ii. PVC Target – Francois has picked up where Robert left off
iii. A-modem mount
iv. Need a swivel
v. Anchor, risers, shackles…etc.
c. Electronic design 
i. Electrical test/power measurement of camera stuff and relay today or tomorrow.  Followed by a final power budget and locked-down design
d. Mechanical design is at the same point – close but not done
i. Need to finalize and order final electrical components
4. Software
a. Code conversion is done
b. Still chasing bugs  
c. 
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