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Quotation – Prop/Duct Project
We are pleased to submit this proposal for your acceptance.  We propose to make high precision Master Models, the first set of your parts, using ARRK's Stereolithography equipment and capabilities.  We will utilize our Stereolithography apparatus to produce the finest and closest reproductions of your products' design using Cibatool material, an Epoxy based photopolymer material.

The second step of our process is to make high-precision cast parts by utilizing the stereolithography Master Models to cast precision silicone rubber molds.  These proprietary molds will then be used to produce high quality duplications of your products using one of ARRK's special thermoset materials.  These Vacu-pressure Moldings are produced in special vacuum chambers with low pressure injection and will provide you with the finest functional prototypes available in the industry.  These parts will duplicate every detail of the Master Models which themselves are precise reproductions of your products' designs.

We are quoting using our exclusive, SUPERCAST material which is a special epoxy based, temperature and impact resistant, color adaptable, thermoset.

SUPERCAST has numerous exciting benefits - it is the closest prototyping thermoset material to ABS and it withstands both higher heat and impact than other prototype casting materials.   In addition to the durability benefits, our SUPERCAST material also allows you to have your color(s) and texture(s) molded right into the parts and,  just like production parts, there's no paint to wear off.

Use ARRK's SUPERCAST material and your product's prototypes can have: 





SYMBOL 183 \f "Symbol" \s 10 \hheat resistance





SYMBOL 183 \f "Symbol" \s 10 \himpact resistance





SYMBOL 183 \f "Symbol" \s 10 \hcolor molded in





SYMBOL 183 \f "Symbol" \s 10 \htexture molded in

Now your products can be the closest replication of production molded parts.

Item
Quantity

Description

Unit Price

Total Price
SLA Master Models

1.   
1
Propellerclock2  - SLA
$1785.00
$1785.00

2.  
1
Colstruct  - SLA
$4360.00
$4360.00

Model Prep

1.
lot
Model Prep
$540.00
$540.00

SuperCast Epoxy Castings - In Color
1.   
2
Propellerclock2  - SC3
$1260.00
$2520.00

2.  
2
Colstruct - SC3
$2695.00
$5390.00

Delivery:
SLA -  5 to 5 Business Days



SuperCast Epoxy Castings - 2 Weeks
Terms & Conditions:

1.  If you require faster delivery, please let us know and we will make every attempt to meet your needs.

2.  The above prices are based on the drawings and/or design data provided.  Any changes to these drawings and/or design data or quantities may affect the final pricing and delivery.  All items are F.O.B.: our San Diego, CA factory.  Unless informed prior to shipping, we will send your prototypes via an overnight carrier, and the associated charges will be added to your invoice.  

3.  Our payment terms are Net 15 days upon approved credit.  All payments are to be made in U.S. Dollars.  This quotation is valid for thirty days from the above date.  Prices do not include any applicable sales or use taxes as required by law. If this project is non-sales taxable, please provide your resale number with your Purchase Order (some states require our obtaining a resale card with the first order and every year thereafter).  The title to these products passes to you prior to ARRK’s use of them. 
4.  Master Model tolerances on dimensions you specify as critical (highlighted or encircled) are (.005".  Casting tolerances will be +/- 0.3% of the Master Models’ overall dimensions due to process factors. 

5. If you supply us with Stereolithography or machined/fabricated Master Models made by another vendor, we cannot be responsible for their ability to produce quality duplications (some vendors use surface finishes that negatively react to silicone rubber molds).  Our quote includes finishing of the exterior surfaces of these Master Models in order to produce Vacu-pressure moldings that are of the highest quality.  

6.  It is ARRK policy to guarantee the production of 10 epoxy parts per silicone rubber mold on the first order.  This policy enables ARRK to produce the highest quality Vacu-pressure moldings (duplications) available.   Stereolithography parts, when used as Master Models in the creation of silicone rubber molds, are typically broken or damaged during their removal from the molds.  For this reason, we cannot be responsible for SLA part breakage occurring during the de-molding process.  This may also necessitate our requiring additional Stereolithography Master Models to produce additional molds and/or parts.

Thank you for your interest and consideration.  We look forward to working with you on this project.  Please direct your order to ARRK Creative Network Corporation.

Respectfully submitted by:





Accepted (Client) by:

Orion Sylvester


Technical Advisor
________________________

650.652.0756 direct
Signature *

orion@arrk.com e mail
Date:       ____/____/____

 * By signing above, I certify that I have my company’s authorization to purchase items indicated on this quotation on behalf of my company.  I hereby authorize ARRK Product Development. to perform the work described herein for the prices indicated.  This signed quotation will be used as a substitute purchase order until ARRK receives my company’s formal, written purchase order.
Note name of file and where it’s stored at bottom end of every document by using forward slashes between directory names (example:  /Dan/quotes/1234-0 means this document, quote #QN01234-0, is saved in the sub-directory called quotes which is a sub-directory of quotes, which is a sub-directory of Dan, which is a sub-directory of Word.  You’ll need to create all necessary sub-directories -- do not save everything in one or two or just a few sub-directories -- you’re asking for computer trouble if you do.  This is “HIDDEN TEXT” and will not print.
