R/V Paragon SPOT beacon

1) "OK" – Automatic position update
    This message is the one that MBARI tampered with for the Stella Beacons and it sends an OK message to drifters@mbari.org every 10 minutes.  I will not have this activated on ODSS because we currently use the AIS at 2 minute intervals.  Running both would make a mess on ODSS.  
    The updated position of the vessel, however, can be accessed through this link:
 http://share.findmespot.com/shared/faces/viewspots.jsp?glId=0mFiNsYzyoQG87f2eMPr4TfBHgGMtt1eH

2) "Custom" - No Emergency
Purpose:  Notify MBARI that everything is OK in the event that cell phone and VHF aren't working.  For example, if the Float Plan time is exceeded but cell service is lost and VHF is unsuccessful.

Message: "Everything is okay, please monitor our position on ODSS"

Recipients: Mike Kelly, Chris Grech, Craig Dawe, Chris Wahl, Jared Figurski

Action: Check the float plan in the manifest box and notify the shore contact that everything is OK and continue monitoring the vessel on ODSS.

3) "Help" - Not life threatening, but require assistance
Purpose:  This message can be sent to request a tow when cell and VHF are not effective.  This is used in a non-life-threatenting situation only.  

Message: "Not a life threatening situation, but we will need a tow.  Call Vessel Assist on VHF 16 or 800-391-4869

Recipients: Mike Kelly, Chris Grech, Craig Dawe, Chris Wahl, Jared Figurski

Action:  The best course of action is to call Vessel Assist and relay the latest position to them.  Our account is #20049361 and is under Jared Figurski.

4) "SOS" - Life Threatening
Purpose:  This will only be used in a life threatening situation, including but not limited to medical conditions and imminent danger (e.g. fire, sinking)

Action:  The SOS message is received by GEOS and rescue is coordinated through IERCC.  Emergency Contacts (Mike Kelly and Jared Figurski) will be contacted to verify that it is not a false alarm.

Message: No message is associated with SOS.

[bookmark: _GoBack]Recipients: GEOS
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