SES 2024B deployment

Recovery- TT drifted out of view when we were recovering SES and ROV. Was very hard to find. Both instruments need flags!!

TT modem small leak but guts were dry. Had tiny pressure release and a small amount of water during housing opening

TT controller did not leak, but did have two screws corrode significantly. Looks like screws and washers were not titanium. Luckily all okay inside. Phew!!

Beacons were not reporting consistently. SES RDF worked. SES strobe worked. Nothing on TT worked. Testing next day showed inconsistencies in argos beacon reporting. Still testing
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