Pre-Deployment Checklist
For clock sync:
ssh: sintela@192.168.1.236
user: sintela
password: 5intela_440
Instrument set-up
· Check Engineering set-up (decimator, leakycutoff frequency settings). If changes are made need to click save chain in the top right of the page.
· Check that correct optical set-up configuration is applied and automatically applied on reboot.
· Check noise floor is reasonable.
· Run OTDR to make sure there is no significant energy loss along cable or reflection at termination. Make sure recorders are off before running.
· Check that GPS time setting is correctly enabled/disabled.
· Check that there is sufficient memory storage available.
· Check that recorders are set-up and files are being recorded to the right place.
· Check RAID is active (especially after deleting files, may need to configure again).
Instrument test via deck cable
· Install shortening plug.
· Start power. 
· Confirm communication with DAS (ping, login to Sintela dashboard).
· Remove deck cable and plug in DeepSea Connect can.
Instrument test via DeepSea Connect (DSC)
· Remove zipties binding DSC can.
· Test communication to “ROV”.
· Engage magnet to turn DSC can on.
· Test communication with DSC can.
· Test communication with DAS.
· Disable DSC can by pushing ROV handle in.

MOB Day
· Test instrument via deck cable (see above).
· Test instrument via DeepSea Connect (see above).
· Test recorders.

Pre-Dive
· Test instrument via deck cable and check set-up (see above).
· Synchronize time.
· Confirm shortening plug has o-rings and is in place.
· Connect batteries.
· Verify working, start recorders.
· Turn off power supply. Verify working.
· Close application.
· Disconnect deck cable.
· Test instrument via DeepSea Connect.
· Test DSC ROV side working.
· Make sure recorders are on.
· Confirm all connectors are snug and all cables are tied up.
· Confirm DSC ROV handle is in off position.
· Confirm deck cable is removed and DSC can is plugged in.
· Check comp levels.
· Turn on sensors (e.g. RF beacon and strobe) and pull any safety pins (e.g., drop weights)

