Notes on how to download data from onyx drives

Use the machine Oldstardust – this runs Linux
Login : geosense
Pwrd: Sintela!

Plug in USB cord of drive
Click icon with multi-disk drive (the icon for the raid drive) to open “Files” in Linux, this mounts the drive
Click on the folder you are interested- “Norway experiment”
The data should be in the “decimator” folder, these should be .raw files each no more than 500 MB
Hook up back up drive into another USB port on Oldstardust
Click on the SSD, to open Files window
Then click on top folder “Norway experiment” then you can copy with ctrl+c and ctrl+v.

Once you are done you can unmount the drive by clicking on the raid or ssd icon and then click “unmount”. 

To check if drive is being loaded
Open Cmd terminal
>sudo tail -f  /var/log/syslog
Then enter password: Sintela!
Hit return, you should see the system log and see if something is mounting

Open platform manager from task bar, make sure it is running
[bookmark: _GoBack]Click to open UI this will open software to view






