16th May 2023

•	Users:
o	Oregon State (Meghan Winground)
o	Washington University
o	WHOI (Maddison Smith)
o	Oxford
•	1.5 pico strain can be detected
•	Dynamic range of 135
•	Switch on/off possible
o	2 minutes to reswitch on
•	No computer is required
•	Cartoon 2 can acquire data but not record
•	Data storage issue can be addressed
•	Box – self-trigger – (based on amplitude or frequency)
•	Sintela does not produce cable