5th December 2024 

Team: Johann Voitglander, Roman Marin, Eric Fitzgerald, Ben Jansen, Charlie Paull, Roberto Gwiazda, Aaron Micallef

Data loggers:

10 kHz
TX1: 159 (new battery)
TX2: 160 (new battery)
Boat: 162

	Time (local)
	Activity

	9.12 a.m.
	Start deployment, 1.5 kn

	9.14
	Tail buoy in water

	9.16
	Stopped deployment to attach first data logger

	9.38
	Second buoy in water

	9.39
	First data logger in water

	9.47
	Data logger back on board due to issues with lines

	9.49
	Data logger back in water

	9.55
	Data logger recovered again

	10.01
	Data logger in water

	10.26
	Second data logger in water, buoy in water

	10.40
	Captain following 15 m isobath

	10.42
	Switch from blue to black winch

	10.45
	First metal sphere attached

	10.50
	First metal sphere in water, buoy in water

	
	TSUNAMI WARNING

	11.04
	Second metal sphere attached

	11.05
	Second metal sphere in water

	11.14
	Payout completed (0.5 nm from starting point)

	11.16
	Start survey at 36°53.428 N, 121°50.785 W, 1.7 kn 

	3.15 p.m.
	Started  slight turn to avoid a buoy. Blue cube at 40°C

	3.45
	End survey at 36°57.306 N, 121°56.868 W

	3.54
	Black cable (connected to transmitter) wrapped around black winch

	3.57
	Started recovery of thick black cable

	4.01
	First sphere draining

	4.03
	First sphere on deck

	4.10
	Recovery at 0.5-0.8 kn

	4.16
	Second sphere draining

	4.19
	Second sphere on deck

	4.24
	Switch from black to blue winch

	4.40
	First data logger on deck

	4.47
	Second buoy of first data logger on deck

	5.04
	Second data logger on deck

	5.09
	Second buoy of second data logger on deck

	5.14
	Tail buoy on deck, recovery complete
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